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SHARP 
	SHARP
	GENERAL
	Drum Won't Spin
	Rubber "o"ring Loose Inside Remove Head Drum Assy And Remove .....Don't Force....

	SHARP
	VC200
	Mode Cogs Go Out Of Alignment.
	Pin Missing In Brake Slide.

	SHARP
	VC2300
	Drum Rotates Very Fast At All Times Operate Is On.
	Suspect Ic706, M51724p, On Servo Pcb.

	SHARP
	VC2300
	Machine Dead With Tape In Laced Up Position.
	Check Q914 (2sa770) On Servo Board O/c.

	SHARP
	VC2300
	No Capstan Drive
	L701 O/c Servo Pcb Rtrnz0012gezz

	SHARP
	VC2300
	No Capstan Drive.
	L701 O/c On Servo Pcb. Pt No: Rtnz0012gezz.

	SHARP
	VC2300
	No Power Ac Adaptor Fails
	Q3 Q4 2sc2826

	SHARP
	VC2300
	No Power, Ac Adaptor Fails.
	Q3 And Q4. 2sc2826 Use Original Parts.

	SHARP
	VC2300
	Pause, Stop & Record Leds All Lit. With No Deck Functions.
	Check Ic807 By Replacement. Check Loading Motor Chip Ic808 And Loading Motor Should Draw 100ma.

	SHARP
	VC2300
	Problems With Rewind
	Change Reel Motor.

	SHARP
	VC2300
	Sound Fluctuating
	Check Capstan Motor Faulty.

	SHARP
	VC330
	Poor Wind And Rewind Playback Ok.
	Check Aux. Brake Not Releasing Because Ic901 Faulty.

	SHARP
	VC330
	Reel And Capstan Motors Going Backwards.
	Change Ic711

	SHARP
	VC3300
	No Channel Indicator, No Go.
	No 12v At Tp901. Check Q904, Q902, Q903, On Pwb-p.

	SHARP
	VC3300
	No Tuner Function And Channel Indicators Not Functioning.
	Replaced Transistor Q904 And C903 On Pwb-p.

	SHARP
	VC3300
	Reel Motor Too Fast Causing Tape Speed To Increase.
	Q863 Shorted, Also Replace Reel Motor If "02" Type.

	SHARP
	VC3300
	Tuner Faulty, Wont Tune In Stations.
	Check For 31.5v On Pin 5 Of Plug Ic. If Faulty Check Function Of Zener Ic201, Ix0037ce, On Pwb-1.

	SHARP
	VC3300
	Won't Tune Stations.
	Ic201 (31v Zener) Rhix0037cezz.

	SHARP
	VC381
	Audio Low Volume.
	Change D606 Leaky Is119.

	SHARP
	VC381
	Cassette Door Opens Only Half Way On Eject.
	Lid Lever Angle Assembly Bent. Rebend To Work.

	SHARP
	VC381
	Clock Will Not Reset.
	Change Mp2812 Under Display Panel.

	SHARP
	VC381
	Dew Sensor Problems
	Change R801 47k Ohms With 470k

	SHARP
	VC381
	Drum Servo Faulty On Record
	Q702,q703 Buffer Osl 2sa945

	SHARP
	VC381
	F901 Or F902 Blows, Int Failure To Rewind Int Tape Spillage
	Check Worn Idler If Ok Reel Motor Suspect.

	SHARP
	VC381
	Intermittent Or No Eject.
	Ic803 (m54532p)

	SHARP
	VC381
	Intermittently Stopping On Play Or Rec., Chewing Tapes.
	Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).

	SHARP
	VC381
	Low Audio
	D606 Leaky Iss119

	SHARP
	VC381
	No Capstan Drive In Record Mode.
	D612 On Audio Board Pwb-b Measures Ok But Is Leaky. Is119.

	SHARP
	VC381
	No Chroma In Rec Or Pb
	Fl501 Rmptd0131gezz

	SHARP
	VC381
	No Colour On Play Or Record.
	Fl501 (rmptdo131gezz). Also Check Fl503

	SHARP
	VC381
	No Eject.
	Change Ic803 (vhim54532p/-1)

	SHARP
	VC381
	No Functions 4 Amp Fuse Blown.
	Check 12 Volt Supply If High (18v) Reg Transistor S/c. make Sure Replacement Is Mounted Correctly On Heatsink (original Is Not).

	SHARP
	VC381
	No Go - 2.5 Amp. Powerfuse Blown.
	Check/ Replace Reel Motor - Always Change Reel Motors With Type Numbers Ending In 02.

	SHARP
	VC381
	No Replay Audio Ee Audio Ok
	C621 S/cct (100uf 25v)

	SHARP
	VC381
	No Video On E-r Mode.
	Check Ic309 For O/c - Or C206 For S/c.

	SHARP
	VC381
	No Video On Playback
	Change Ic308.

	SHARP
	VC381
	Not Erasing Previous Audio Track.
	Audio Cable Shorted Under Plastic Tie Near Audio/ctl Head.

	SHARP
	VC381
	Picture Rolling On E-e And Record.
	Change C438 47 Mfd, C439 (nearly O/c). If Ok Check Around Ic201 And Ic402.

	SHARP
	VC381
	Playback In Colour Will Not Record In Colour.
	Check Fl503. The Down Converted Signal Should Be 500 millivolt P-p On Pin 1 Of Colour I.C. The Carrier Signal Should Be 500 Millivolt P-p At Pin 28.

	SHARP
	VC381
	Remote Erratic.
	C811 (.01 Uf) Leaky.

	SHARP
	VC381
	When Play Is Selected Squeaking From Head Drum, Then Stops.
	Change Reel Idler

	SHARP
	VC381
	When Record Is Selected Machine Fails To Stay In Record.
	Check T/u Reel Not Turning In Record Mode. Playback Ok. Change Ic7754.

	SHARP
	VC381
	When Replacing Cass Lamp, To Check Correct One Is Fitted. .
	Check Voltage R872-5. Check Voltage On Point Where Ic802 And R872-5 Connect, Should Be 8 Volts If Lower Wrong Cass Bulb Has Been Used.

	SHARP
	VC381
	Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
	Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.

	SHARP
	VC381X
	No Record Colour.
	Replaced Filter Fl503.

	SHARP
	VC381X
	Take Up Spool Not Rotating In Record. Ok In Playback.
	Change Ic7754.

	SHARP
	VC381X
	When Pic. Search Is Selec. Mach. F/f Or Rew.
	Check For 9.9v On Pin 32 Of Ic801. Change Ic801, D7758 If Still Present Check Ic805 And Ic806 If Ok Check Pins 1,4,5 Of 17754 Go High In Search Mode And Pins 12, 13, 16 Go Low. If D7753 Cathode Is Not High At This Time, Change Q7751 If Pin 59 Of Ic801 Do

	SHARP
	VC383
	Intermittently Stopping On Play Or Rec., Chewing Tapes.
	Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).

	SHARP
	VC383
	Low T/u Torque.
	Adjust R7765 "tu Torque".

	SHARP
	VC383
	No Video On E-r Mode.
	Check Ic309 For O/c - Or C206 For S/c.

	SHARP
	VC383
	No Video On Playback
	Change Ic308.

	SHARP
	VC383
	Refer Vc381
	 

	SHARP
	VC383
	Self Rec. Tapes, Band Few Lines Deep,third Way Down.
	Check Record Switching Monostable Faulty, Check C714 And Reel Motor And Idler.

	SHARP
	VC383
	Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
	Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.

	SHARP
	VC386
	Audio Click In P/back. Usually Only 1 Channel.
	Rh-1z0038ge. Need Switch Ic Audio.

	SHARP
	VC386
	Audio Low On One Channel
	Replace Ic651 Rh1z0038gezz

	SHARP
	VC386
	Audio Low On One Channel Of Own Record.
	Change Ic Rh120038gezz.

	SHARP
	VC386
	Audio Low On One Channel.
	Replace Ic651 (rh1z0038gezz).

	SHARP
	VC386
	Blank Screen On Play And Tuner.
	L 409 (220 Uh) On Video Pcb.

	SHARP
	VC386
	Blank Screen On Play Or E-e.
	No 12v On Pin5 Of Ic402. Check L407, L409 On Video Pcb.

	SHARP
	VC386
	Capstan Fails To Start
	D6605

	SHARP
	VC386
	Clock Flashes & Returns To Ch1, As If Power Was Interrupted
	Replace All Electro's In Psu.

	SHARP
	VC386
	Clock Flashes And Resets To Ch1 As If Lost Power
	Replace All Electros In Psu, Specifically C16 (10uf 50v)

	SHARP
	VC386
	Drum Rotating Too Fast.
	Chek C710 S/c.

	SHARP
	VC386
	Flickering Colour
	Fl503 Rmptd0052gezz

	SHARP
	VC386
	Flickering Colour.
	Fl503 (rmptd0052gezz).

	SHARP
	VC386
	Flickering Colour.
	Change Filter Fl503. Rmpdt0052gezz.

	SHARP
	VC386
	Int No Function Of Channel Change.
	Check For D/j On Socket Ta On Pwb.

	SHARP
	VC386
	Interm. Colour In P/back Or Rec. No Colour In P/back Rec.
	Replace Fl503.

	SHARP
	VC386
	Intermittently Stopping On Play Or Rec., Chewing Tapes.
	Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).

	SHARP
	VC386
	Low Sound
	Q6601 (bc337) Pin 3 Bi 8.5 Volts.

	SHARP
	VC386
	No Colour In Record
	Ic501 Ha11781nt, Fl503 Rmptd0052gezz

	SHARP
	VC386
	No Colour On Record.
	Ic501 (ha11781nt) Or Fl503 (rmptdoo52gezz)

	SHARP
	VC386
	No Picture In Pb Or Ee
	L409 220µh ,l407 On Video Pcb.Check 12v Pin 5 Ic402

	SHARP
	VC386
	No Power And Audio Pcb
	Check C/protector On M/board Near Tracking Control (12v)

	SHARP
	VC386
	No Video On E-r Mode.
	Check Ic309 For O/c - Or C206 For S/c.

	SHARP
	VC386
	No Video On Playback
	Change Ic308.

	SHARP
	VC386
	Poor Colour Saturation On Still Of Pre-recorded Tapes.
	Change R429 To 1k Ohm On Y/c Pcb.

	SHARP
	VC386
	Traking Control No Effect.
	Tracking Control O/c.

	SHARP
	VC386
	Tuning Drift All Channels.
	Check D1430 On Tuning Board Leaky. Also D1425 - 1444.

	SHARP
	VC386
	Tuning Drift.
	Check Pr01 Regulator Also Ic1403 Or Int Tuning Pots.

	SHARP
	VC386
	Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
	Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.

	SHARP
	VC386..
	No/int Reel Drive.
	Ic705 Ta7267p.

	SHARP
	VC387
	Faulty Audio
	Protector Ic619 On Audio Pcb O/c Icp-n10

	SHARP
	VC387
	Faulty Audio.
	Protector Ic619 On Audio Pcb O/c. Icp-n10.

	SHARP
	VC387
	Intermittently Stopping On Play Or Rec., Chewing Tapes.
	Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).

	SHARP
	VC387
	No Drum Rotation.
	14 Volt Supply Fuse O/c Not Shown On Cct.

	SHARP
	VC387
	No Power On, Clock Ok.
	Check For 9 Volt On Pin 64 Of Ic801, If Not, Look For O/c Semiconductor Fuse Not Shown On Cct.

	SHARP
	VC387
	No Tuner, Blank Screen.
	Check R954 (2.2 Ohm) And Check Q953, Q954, And Electro's In Psu.

	SHARP
	VC387
	No Tuner. Blank Screen
	Check R954 2.2 O Q953 Q956, Q955 & Electros In Psu

	SHARP
	VC387
	No Video On E-r Mode.
	Check Ic309 For O/c - Or C206 For S/c.

	SHARP
	VC387
	No Video On Playback
	Change Ic308.

	SHARP
	VC387
	Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
	Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.

	SHARP
	VC387
	Won't Operate.
	Protector Ic815 On Mecha Cont Pcb. Icp-n5.

	SHARP
	VC387
	Wont Operate
	Proctector Ic815 Icpn10 Mecha Pcb

	SHARP
	VC388
	Intermittently Stopping On Play Or Rec., Chewing Tapes.
	Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).

	SHARP
	VC388
	No Colour In Play
	Replace X502 4.433 Mhz Adjust

	SHARP
	VC388
	No Colour On Play.
	Replace 4.433 Xtal. (x502) - Adjust Frequency.

	SHARP
	VC388
	No Functions.
	Check Q5002 S/c Because Ic15002 S/c.

	SHARP
	VC388
	No Go
	Q1 2sc2625, Ic1 Pc511n

	SHARP
	VC388
	No Power. No Clock. No Functions
	Q5002 O/c No +5v Rail. Aprox Load Current 90-100 Ma

	SHARP
	VC388
	No Video On E-r Mode.
	Check Ic309 For O/c - Or C206 For S/c.

	SHARP
	VC388
	No Video On Playback
	Change Ic308.

	SHARP
	VC388
	Power No Go.
	Q1 (2sc2625) And Ic1 (pc511n).

	SHARP
	VC388
	Power Supply Faulty After Fitting A New Capstan Motor.
	Check: Q1 (2sc2625) Chopper Ic1 Pc511n. Also Change C7022 To (1 Mfd 50v) R7040 To (27k Ohms)

	SHARP
	VC388
	Power Supply Wont Start Reliably
	Reduce Value Of R32/r57 To 27r Instead Of 54r

	SHARP
	VC388
	Snowy Or Flyscreen Effect On Own Recording.
	Reduce Chroma Record Current.

	SHARP
	VC388
	Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
	Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.

	SHARP
	VC388
	Won't Load Tape.
	I 806 (s16900a).

	SHARP
	VC388
	Wont Load
	Ic806 Si6900a

	SHARP
	VC390
	Black Streaks In Playback
	Heads Ok, Check 3.8 Mhz Oscillator Is Not Running At 5 Mhz.. C227 Intermittent Replace. Readjusting Will Not Repair The Fault

	SHARP
	VC390
	Int Wont Record Picture
	Q204, Q205 2sa733

	SHARP
	VC390
	Intermittently Stopping On Play Or Rec., Chewing Tapes.
	Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).

	SHARP
	VC390
	Locked In Lp Or Sp Frontpanel Ctrl Won't Affect.
	Check Sw8001 And Sw8002 Are Inthe Mid Position.

	SHARP
	VC390
	Looks Like Video Heads, Black Streaky Lines In Playback
	Replacing Heads Didnt Fix . The Problem Was The 3.8 Mhz Fm Oscillator Was Running Naer 5mhz. Trimmer Cap C227 Intermittent. Readjusting It Worked, But It Has To Be Replaced. to Adjust The Free-run Freq, Put Vcr In Line In Mode And Place A Frequency Coun

	SHARP
	VC390
	No Picture In Play
	Ic308 Protector Icp N10

	SHARP
	VC390
	No Video On E-e Mode.
	Check Ic309 For O/c - Or C206 For S/c.

	SHARP
	VC390
	No Video On Playback.
	Change Ic308.

	SHARP
	VC390
	Poor Record Looks Like Stuffed Heads.
	C227 Possibly Faulty( Fm Freq) Adjust And Return To Previous Setting To Check.

	SHARP
	VC390
	Poor Recording
	Ry301 Contacts Dirty - Clean And Replace.

	SHARP
	VC390
	Shuts Down After 30 Mins.
	Replace C12 In Power Supply 220uf 16v

	SHARP
	VC390
	White Lines/dots In Play
	C17 220µf/16v In Psu

	SHARP
	VC390
	Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
	Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.

	SHARP
	VC390
	Will Not Eject Tape.
	Check Lever On Rhs Of Eject Mechanism Activates Micro Switch Clean And Service.

	SHARP
	VC468
	Int Picture Rolling On Playback.
	Check R743 Has No Effect If So C725 Gone O/c.

	SHARP
	VC481
	Capstan Fails To Start
	Mode Switch

	SHARP
	VC481
	Capstan Fails To Start.
	Mode Switch. Qsw-r0010gezz.

	SHARP
	VC481
	Capstan Slow In Play/rec
	D742 Servo Pcb

	SHARP
	VC481
	Capstan Slow In Play/rec.
	D742 On Servo Pcb.

	SHARP
	VC481
	Capstan Unlocked.
	Check Tracking Control For Dry Joints.

	SHARP
	VC481
	Capstan Won't Lock Even After Replacing, Motor, Bearing, And Doing A Lock Adjustment.
	Check For Spikes On Control Track Signal. If So Replace Capstan Servo Chip(ic702)

	SHARP
	VC481
	Cassette Inject Faulty.
	Won't Open Door Of Cassette. Change Slider Assembly. Lhldx3016gezz.

	SHARP
	VC481
	Chews Tapes No Rewind
	Q8022 Phot Transistor Px0053gezz

	SHARP
	VC481
	Chews Tapes, No Rewind.
	D734 Leaky, Off Pin 10 Of Ic 708 On Pwb-a.

	SHARP
	VC481
	Goes Into Rewind.
	Q8022 Photo Transistor. Px0053gezz.

	SHARP
	VC481
	Interm Reel Motor Drive.
	Check For Dry Joints On Q713.

	SHARP
	VC481
	Interm. Capstan Motor Drive.
	Check For Dry Joints On Q708.

	SHARP
	VC481
	No Capstan Lock.
	R794 (4.7k). Put Another 4.7k In Parallel. On Capstan Servo Pcb

	SHARP
	VC481
	No Or Flickering E-e Pic. In Stop Mode Pb. 9v Is 3v S/b 0v.
	Ic802 (ir2403 Or Td62105) Faulty.

	SHARP
	VC481
	No Reel Drive
	Ic708 Faulty Placing 3v Dc On Reel Drive Switch Input (ic705,p2)

	SHARP
	VC481
	Operation Light Not On.
	Change Protector Pr801 Qfs - P1021gezz. Change Q813 2sc945 On Mechanon Board Pwb-e. C452 S/c On Y/c Board, Also Check Pr-eb Protector On Pwb-e.

	SHARP
	VC481
	Picture Flickering In Ee
	Pb9v Rail Is 3volts. Ic802 Ir2403/td62105

	SHARP
	VC481
	Won't Accept Tape.
	Slider Assy. Lhldx3016gezz.

	SHARP
	VC481
	Won't Accept Tape.
	Cassette Switch On Cassette Carriage O/c. Qsw-f0010gezz.

	SHARP
	VC481
	Won't Tune Stations.
	Ic951 On Power Supply Pcb.

	SHARP
	VC481
	Wont Accept Tapes
	Carrige Switches Qsw F0010gezz

	SHARP
	VC481
	Wont Accept Tapes
	Slider Asy Lhldx3016gezz

	SHARP
	VC481
	Wont Tune Channels
	Ic951 In Psu

	SHARP
	VC482
	Play Selec. Goes Into F.F Search. Own Rec. Ok On Other Mach
	Check Pin 5 Of Ic802, If Not Zero Volts Change Ic802.

	SHARP
	VC482
	Refer Vc481.
	 

	SHARP
	VC482
	See Sharp Vc481
	 

	SHARP
	VC482
	Wont Record Or Erase Sound.
	Check If Q603 (2sc2001) Leaky.

	SHARP
	VC483
	Power Supply O.K. But No Display Or Functions.
	Pr801 Fuseable Resistor Faulty.

	SHARP
	VC483
	See Sharp Vc481
	 

	SHARP
	VC483
	Tape Counter Not Working
	Check For Obstructions To Auxiliary Pulse Generator Wheel.

	SHARP
	VC486
	Clock Gains 10mins/day. C5007 Wont Adjust Tp2 To 131.072khz
	C5006 (10pf) In Parallel With Trimmer O/c.

	SHARP
	VC486
	Clock Runs Fast
	Adjust Tp2 For 131.072khz If Not C5006 O/c

	SHARP
	VC486
	Counter Erratic
	Photo Sensors Faulty Or Need Clean

	SHARP
	VC486
	Counter Numbers Erratic.
	Q8004 And Q8005 Photo Interrupters Faulty.

	SHARP
	VC486
	Counter Problems.
	Change 2x Photo Interrupters.

	SHARP
	VC486
	Cyclic Noise Bar On Play
	Check C743 100uf 16v Cap. (bias Bypass For Control Track Pulse Amp.

	SHARP
	VC486
	Erratic Behaviour Of Deck.
	Check Faulty Mode Switch.

	SHARP
	VC486
	Faulty Load/unload In P/back & Rec. Interm.Changes Mode.
	Change Mechanism Position Switch. Qsw-r0008gezz.

	SHARP
	VC486
	Goes To Stop Just As It Fully Loads.
	Drum Pg Coil O/c. On Lower Drum Under Rotary Tx.

	SHARP
	VC486
	Int Changes Mode, Chews Tapes
	Mode Switch Qsw R0008gezz

	SHARP
	VC486
	Int Changes Mode, Chews.
	Mode Switch. Qsw-r0008gezz.

	SHARP
	VC486
	Int Cuts Out In Pb
	Replace Reel Sensors

	SHARP
	VC486
	Int Cuts Out In Play/record After 1 Hour.
	Replace Reel Sensors.

	SHARP
	VC486
	Int Picture Rolling On Playback.
	Check C725 On Servo Board.

	SHARP
	VC486
	Interm. Cuts Off On P/back Or Rec After I Hour Approx.
	Change Reel Sensors - Photo Interrupters Rh-px0042gezz.

	SHARP
	VC486
	Method Of Adjusting Capstan Servo Lock.
	Short Ends Of D763. Adjust R777 To Give 3.6v At Pin 5 Of T.P.B. When Short Is Removed Voltage May Change Though Should Remain Stable.

	SHARP
	VC486
	Mod. To Prev. Overheating Ic714 In Servo Circuit.
	On Track Side Of Servo Pcb Place A 100 Ohm .5w And A 10 Mfd 16v Electro In Series From Emitter Of Q717 To Pin 8 Of Ic714.

	SHARP
	VC486
	No Clock, No Functions. Tuning Stuck On Ch O.
	X5001 Faulty Or Ceramic Caps On Track Side Of Pcb Causing Shorts.

	SHARP
	VC486
	No Clock, No Go, Wont Change Channels
	X5001 Or Cermac Caps Shorting On Pcb Side.

	SHARP
	VC486
	No Colour In Pb Or Rec
	Q501 2sc2308

	SHARP
	VC486
	No Colour On Play/record.
	Q501 (2sc2308) Faulty.

	SHARP
	VC486
	No Functions.
	Capstan Mtr Ic And Micropocessor Ic .Suspect Capstan Mtr.

	SHARP
	VC486
	No Functions.
	Microprocessor, Capstan Drive Ic Shorted, Suspect Capstan Motor.

	SHARP
	VC486
	No Load/eject
	Ic808 Ta7267

	SHARP
	VC486
	No Reel Drive
	Ic810 Ta7267 Q826,q827,q828

	SHARP
	VC486
	No Reel Drive.
	Ic810 (ta7267p/-1) And Check Q826, Q827, Q828.

	SHARP
	VC486
	No Reel Motor Drive.
	Change Ic810 (ta7267p/-1). Check Q826, Q827, Q828.

	SHARP
	VC486
	No Remote Control.
	Check Ic812 (lr3711m/-1). Check Possible Faulty Mode Switch.

	SHARP
	VC486
	Operation Light Not On
	See Same Fault Vc481 Above.

	SHARP
	VC486
	Reel Motor Wont Turn When Laced Up And Playing. Tape Stuck
	Change Ic715 On Pwb-a Vhiba6209//-1.

	SHARP
	VC486
	Rf Inter. On P/back. Could Be Vcr To Close To Tv Transmitter
	1. On Pwb-x Head Amp. Board Cut Tracks On Pins 6 & 8 Of Ic3301. Place A Ferrite Bead Of 4 Turns Across Each Track. 2. Add 180 Pf Capacitors From The Audio In And Out Rca Sockets To Earth. Hardwire Input Board Gnd. To Power Supply Gnd.

	SHARP
	VC486
	Tape Counter Counting Faulty.
	1. Check The Lower Reflective Surface On The Counter Relay Pulley On Top Deck Of Mechanism. If The Reflective Surface Is Not Perfect - Replace. P.No. Nplyv0088gezz. 2. Check And Clean Photo Interruptor Sensors. P.No.

	SHARP
	VC486
	Vert Jitter Etc On Own Recordings.
	Q711 Heat Sensitive. Head Switching Varies.

	SHARP
	VC486
	Vert Jitter In Self Rec
	Q711 Head Switch Varies

	SHARP
	VC486
	Won't Accept Cassette. Operation Faulty.
	Refer Same Fault Sharp Vc8482. Replace C826, 10µf 16v, On Mecha Control Pcb.

	SHARP
	VC486
	Won't Record Or Play Colour Intermittently.
	Fl505 5.2mhz Filter Faulty.

	SHARP
	VC486
	Wont Load Or Eject Tapes.
	Ic808 (ta7267p).

	SHARP
	VC486
	Wont Turn On
	C532 Shorted On Pwb-c

	SHARP
	VC486
	Wont Turn On.
	Check C532 Shorted On Pwb-c.

	SHARP
	VC488
	Colour Dashes All Over Screen On Play.
	Earth Capstan Drive Ic Heatsink, And Add .01uf From Pin 9 To Earth.

	SHARP
	VC488
	Colour Dashes In Pb
	Earth Capstan Drive Ic H/sink, Add .01µf B/t Pin 9 & Earth

	SHARP
	VC488
	Goes Into Ff, Rew, Stop Etc By Itself.
	Q805 On Pwb-e (2sc174) In Syscon.

	SHARP
	VC488
	Goes To Stop Just As It Fully Loads Up
	Drum Pg Coil On Lower Drum O/c (under Rotary Transformer)

	SHARP
	VC488
	Hifi Light Flickers & Goes Out When Hot Or No Hifi On Play.
	Audio 9v Goes Low, Ic953 95kucz0072gezz. M5230 L Ic On Power Supply Board, Its A Bitch To Get At

	SHARP
	VC488
	Int Changes Mode, Chews Tapes Etc.
	Mode Switch. Qsw-r0008gezz.

	SHARP
	VC488
	Int Goes Into Any Mode By Itself
	C805 Syscon 2sc174

	SHARP
	VC488
	Laces Up Then Unlaces, Drum Turns For Sec. Or Pic Shakes.
	Drum Motor Rmotp1071gezz.

	SHARP
	VC488
	Lines In Pb. Tracking Not Working
	Pots In Drawer O/c Repace

	SHARP
	VC488
	Looks Like Heads Faulty.
	Electros In Psu. C956(1uf), C962(1uf), C957(.047uf).

	SHARP
	VC488
	No Audio No Functions
	Ic5006 Rhix0014gezz Microproccer

	SHARP
	VC488
	No Capstan Lock, No Ctl.
	C776 (100µf/16v).

	SHARP
	VC488
	No Chroma On Play.
	Mn6163 Chroma Ic.

	SHARP
	VC488
	No Reel Drive In Any Mode.
	Suspect Ic715, Ba6209 On Servo Pcb.

	SHARP
	VC488
	No Sound, No Clock Or Channel Display, Ch Buttons Dont Work
	Ic5006 Rhix0014gezz Microprocessor.

	SHARP
	VC488
	Picture Rolls Like Loss Of Capstan Lock. Capstan Servo Adjust Helps But Not Good Enough.
	Replace C776(100uf 16v) Electrolytic Capacitor, On Servo Pcb. (top Left Board). It Was Short Circuit.

	SHARP
	VC488
	Picture Shakes Or Wont Play.
	Drum Motor Rmotp1071gezz

	SHARP
	VC488
	Reel Wont Turn When Fully Loaded Wont Eject.
	Ic715 On Pwb-a. Vhiba6209//-1

	SHARP
	VC488
	See Vc486
	 

	SHARP
	VC488
	Static In Pb. (looks Like Heads)
	Electros In Psu C956, C962 , C963 = 1µf & C957 .047µf c956 In Particular

	SHARP
	VC488
	Stopped In Laced Position.
	Mode Switch. Qswr0008gezz.

	SHARP
	VC488
	Switches On, Switches Off, Laces Up Weird Problems.
	Pcb Behind Timer/clock Display Full Of Dj's Where Leads Connect To Pcb.

	SHARP
	VC488
	Tape Remain Indicator Erratic.
	Reflective Stripes On T/u Reel U/s Or Q903 In Psu.

	SHARP
	VC488
	Tracking Bars On Screen
	C776 100µf In Control Amp

	SHARP
	VC488
	Traking Not Working.
	Check 3 Pots In Drawer, One Or All May Be O/c.

	SHARP
	VC581
	Black Screen In Ee
	Cracked Pcb Near Rf Booster

	SHARP
	VC581
	Black Screen On E-e.
	Craked Pcb Around Rf Booster.

	SHARP
	VC581
	Buzz In Sound.
	Change T1501 Pif.-det. Transformer. New Types 0029.

	SHARP
	VC581
	C/stan Rotates B/wards When Stop Pressed. Stops When Played
	Check Shorting Links J20/j25 Shorting Out On R/h Side Of Mother Board.

	SHARP
	VC581
	Capstan On At All Times. No Reel Motor Drive.
	Check Operation Of Ic706, Bu4011b.

	SHARP
	VC581
	Capstan Speed Varies On Play And Record.
	Replace Ic704. Rh-1x0107gezz.

	SHARP
	VC581
	E-e Picture Distorted.
	Ic1501. (x0275ce).

	SHARP
	VC581
	Ee Picture Is Distorted
	Ic1501 X0275ce

	SHARP
	VC581
	Functions Faulty, No Motor Drives.
	No 14v At Pin 7 Of Plug Pa On Power Supply. Check For Circuit Protector Ip901 In Power Circuit. P.No. 95kpjc285zz.

	SHARP
	VC581
	Goes Into Any Mode As Soon As Operation On.
	Change Q812 Vsdta124es/-1. Should Have 4.5v At Pin 43 Of Ic801.

	SHARP
	VC581
	Intermittent Functions.
	Q812 (dta124).

	SHARP
	VC581
	Looses Drum And Capstan Lock In Play
	Dry Joint On Xtal X501 In Chroma Section

	SHARP
	VC581
	No Colour On Play Or Record.
	Fl501 (rmptdo131gezz). Also Check Fl503

	SHARP
	VC581
	No Go Clock Ok
	Ip901 2.5 Amp O.C In Psu

	SHARP
	VC581
	No Go, Clock Ok.
	Ip901 2.5a O/c In Psu.

	SHARP
	VC581
	No Operate Led
	No Pcon 12 V Check Ic902 M5236l

	SHARP
	VC581
	No Operation Light. Laces Up Then Unlaces.
	Check Ic902 In Power Supply.

	SHARP
	VC581
	No Reel Drive
	Ic702 Ta7267p

	SHARP
	VC581
	No Reel Motor Drive.
	Change Ic702, (ta7267p).

	SHARP
	VC581
	No Tape Functions, No Operate Led.
	Fuse On Psu, P901 2.5 Amp

	SHARP
	VC581
	Operation Faulty.
	Check P.Con. 9v Switch, Q909, 2sc3518 In Power Supply. if Faulty Or Overheating, Check For Short Circuit To Ground On P.Con. 9v Line, Pins 14-15 Of Plug Pa. If Short To Ground, Check For Faulty C219, 100µf 16v, Near The Edge Of Main Pcb, Near Ic 402.

	SHARP
	VC581
	Pause/still Indicator On But Cont. To Play Or Record.
	Remove C8001 (47 Mfd 16v) Pwb-w Across Loading Motor.

	SHARP
	VC581
	When Tuning To Station - Goes To Blank Screen Agc Faulty.
	Change Ic1501

	SHARP
	VC581X
	Wont Play Or F.F. Supply Brake Stuck On.
	Replace Microcomputer Ic801.

	SHARP
	VC584
	Clock On, Won't Operation On.
	Check For Open Circuit Ip902 In Power Supply. P. No. 95kpjc0284zz. Check For Short Circuit Or Faulty C1589, 1000µf 16v, On Tuner Pcb.

	SHARP
	VC585
	E-e Picture Distorted.
	C211 (10 Uf/16v) Inside If Module.

	SHARP
	VC585
	Ee Picture Distorted
	C211 10µf/16v In If Module

	SHARP
	VC585
	Hum And Pattern Interference In Ee And Play. High Freq. Oscillations On +12 & +9v Rails
	Replace C913,917,918,919 And C916 In Power Supply.

	SHARP
	VC6300
	Sound Wowing.
	Check Capstan Motor Speed By Selecting Record And Adjust R794 For Zero Volts On Tp713, If Tp721 Exceed 500 Millivolt P-p Ripple, Change Motor.

	SHARP
	VC6300
	Turns Off While Recording Or Switches Off After 6 Inches.
	Check For Take-up Reel Rotation, Or The Machine Thinks So. Check That The Reel Isn't Stopping - If It Does Clean Belts And Tyres And Replace The Clutch. If The Reel Isn't Stopping Check The Output From The Sensor Af4: It Should Be 5-10v P-p, If Not Repla

	SHARP
	VC651
	Capstan Goes To Half Speed
	Clean Ctrl Track Head With Pcb Cleaner. Low Control Track Forces Capstan Servo To Half Speed Mode.

	SHARP
	VC651
	Capstan Runs Fast In Record
	Diode In Syscon Faulty(leaky) D814

	SHARP
	VC651
	Capstan Too Fast
	Check Fg Pulse Dj's Plug A1

	SHARP
	VC651
	Capstan Too Fast.
	Check Fg Pulse, Dj's Around Plug A1.

	SHARP
	VC651
	Chews Tapes, Intermittent No Take Up Torque.
	Reel Brake Not Releasing, Mode Switch Faulty.

	SHARP
	VC651
	Chews Tapes, Poor T/u Torque.
	Reel Brake Not Releasing. Mode Switch?

	SHARP
	VC651
	Int Capstan Lock
	Cracks Around Screws Holding Pcb-a

	SHARP
	VC651
	Int Capstan Lock.
	Craks Around Screws Holding Pcb-a.

	SHARP
	VC651
	See Vc685
	 

	SHARP
	VC651
	Slow Capstan Speed
	Pinch Roller In Engaging. Lubricate Pivot.

	SHARP
	VC681
	Cassette Loads Up & Down At Power On By Itself ?
	R822 Dj's Or O/c On Mother Pcb

	SHARP
	VC681
	Cassette Loads Up And Down At Power On By Itself.
	R822 Dj's Or O/c On Mother Pcb.

	SHARP
	VC681
	Chews Tapes
	Loading Belt

	SHARP
	VC681
	Chews Tapes.
	Loading Belt Faulty.

	SHARP
	VC681
	Loads Or Eject But No Functions
	End Sensor O/c

	SHARP
	VC681
	No Chroma In Record
	Chroma Delay Line.

	SHARP
	VC681
	No Chroma On Record.
	Chroma Delay Line.

	SHARP
	VC681
	Records Ok ,ee Ok But Mutes Video And Audio
	No Pb 5v. C413 On Luminance/chroma Sub Board S/cct.

	SHARP
	VC681
	See Vc685
	 

	SHARP
	VC681
	Will Load And Eject But No Other Functions.
	End Sensor O/c.

	SHARP
	VC681
	Wont Load Or Eject. Interm Doing Either.
	Reposition The Mode Control Switch.

	SHARP
	VC682
	Capstan And Reel Go Forward In Rewind Mode
	Plug A1 Pin 8 Dj'd

	SHARP
	VC682
	Capstan And Reels Go Forward In Rewind.
	Plug A1 Pin 8 Dj'd.

	SHARP
	VC682
	Capstan Slows Down
	Isolate Pin 13 Of Ic703 And Connect To Earth.

	SHARP
	VC682
	Capstan Slows Down.
	Isolate Pin 13 Of Ic703 And Connect To Earth.

	SHARP
	VC682
	No Functions
	R916 O27 In Psu

	SHARP
	VC682
	No Functions.
	R916 (.27 Ohm) In Psu.

	SHARP
	VC682
	No Load Motor
	Ic802 Ta7288

	SHARP
	VC682
	No Load Motor Drive.
	Ic802 (ta7288).

	SHARP
	VC682
	No Play Functions
	Ic801

	SHARP
	VC682
	No Play Functions.
	Ic801 (rh-ix0151gezz).

	SHARP
	VC682
	Won't Load/eject.
	R907 (.27 Ohm) In Psu O/c.

	SHARP
	VC682
	Wont Load/eject
	R907 O27 In Psu

	SHARP
	VC682X
	When In Rec. Pause Mode, Wont Rec.
	Replace Mode Select Switch.

	SHARP
	VC685
	Brakes Don't Lock Hubs On Eject,
	Pin From Underneath Slider Panel Has Fallen Out.

	SHARP
	VC685
	Looks Like Worn Idler
	Brake Solenoid Underneath Plugs Into Reel Sensor Pcb Not Working

	SHARP
	VC685
	No Clock Display
	Ic5001 Pwb-i

	SHARP
	VC685
	No Clock Display.
	Ic5001. (rh-ix0164gezz) On Pwb-1.

	SHARP
	VC685
	No Picture In Playback
	Missing Pb 5v Q808 Replace C413 (100µf/10v) On Y/c Module Board (rhs).

	SHARP
	VC685
	Reel And Capstan Run Backward
	Clock Xtal For Ic801 R/s

	SHARP
	VC685
	Reel And Capstan Run Backwards, Vcr Won't Turn Off.
	Clock Xtal For Ic801 Faulty.

	SHARP
	VC685
	Similar Symptoms To Worn Reel Idler.
	Brake Solenoid Underneath Plugs Into Reel Sensor Pcb Not Working.

	SHARP
	VC685
	Vcr Wont Turn Off
	Clock Xtal Faulty For Ic801

	SHARP
	VC685X
	Wont Eject Tapes Chews Tapes.
	Replaced Filter Fl801.

	SHARP
	VC7300
	Capstan Motor Will Not Operate.
	Replaced Q809.

	SHARP
	VC7300
	Capstan Won't Operate.
	Q809 (2sd687).

	SHARP
	VC7300
	Capstan Wont Operate.
	Q809 (2sd687).

	SHARP
	VC7300
	Capstan Wont Work
	Q809 2sd687

	SHARP
	VC7300
	Cassette Loading Motor On At All Times.
	Check Q8811 2sd687

	SHARP
	VC7300
	Cassette Motor On All Time
	Q809 2sd687

	SHARP
	VC7300
	Cassette Motor On At All Time.
	Q809 (2sd687).

	SHARP
	VC7300
	Cassette Motor On At All Time.
	Q809 (2sd687)

	SHARP
	VC7300
	Chopper Tranformer Squealing
	Change C920 (10mfd 50v)

	SHARP
	VC7300
	Dew Sensor On
	Q805 Q806 2sc1815

	SHARP
	VC7300
	Dew Sensor On All The Time.
	Q805, Q806 (2sc1815).

	SHARP
	VC7300
	Dew Sensor Operating With No Moisture Present.
	Replace Q805 And Q806.

	SHARP
	VC7300
	Dew Sensor Problems.
	Check Q805 And Q806, 2sc1815.

	SHARP
	VC7300
	Drum Rotates At All Times, No Functions.
	Check Loading Ring Position And Reset If Necessary.

	SHARP
	VC7300
	Drum Rotates At All Times, No Inject Or Eject.
	Check Mechanical Loading Ring Position.

	SHARP
	VC7300
	Drum Rotates No Functions
	Check Loading Ring Position & Reset If Necc

	SHARP
	VC7300
	Functions Ok But No Eject
	Lever #23 Rhs Eject Mech Lubricate

	SHARP
	VC7300
	Functions Ok But Won't Eject Tape.
	Lever (no 33 On Parts List) On Rhs Of Front Loader Sticking, Lubricate.

	SHARP
	VC7300
	Ghosting Picture Appears After A Few Hrs. Operation On E-e
	Freeze Sf1501 Filter On Tuner I.F. Board If Picture Comes Good Replace Filter.

	SHARP
	VC7300
	Int B/w Picture On Playback. Audio Ok.
	Check If Main Solenoid Releases When Stop Is Pressed. If Not Solenoid Could Need Lubrication.

	SHARP
	VC7300
	Int Pulsing Of Aux. Motors.
	Change Regulator Trans 2sc1212a To A Bd139 With Moderate Heat Sink.

	SHARP
	VC7300
	Int Recording.
	Check Ic1301 Pin 8 For Int Loss Opf Signals.

	SHARP
	VC7300
	Loading Motor Weak.
	Change Q8091.

	SHARP
	VC7300
	Loading Motor Won't Rotate.
	Look For Thermal Output To Main Solenoid O/c.

	SHARP
	VC7300
	Loss Of Colour On Pre-rec. Playback Of Own Rec. Ok.
	Fit 270 Pf In Parallel With C540. Fit 1.8k Ohms 1/4w In Parallel With R522.

	SHARP
	VC7300
	No 12 V Rail
	R903 O27 Fuse

	SHARP
	VC7300
	No 12 Volts At Tp901.
	Replaced R903.

	SHARP
	VC7300
	No 12v At T.P. 901.
	On Vc7300 Check R903 0.27 Ohms. On Vc7700 Check R912 0.27 Ohms Q904 2sd1128.

	SHARP
	VC7300
	No 12v From Power Supply.
	Check R903 (.27 Ohm Fusible).

	SHARP
	VC7300
	No Capstan Motor Drive.
	Check Q809, 2sd687.

	SHARP
	VC7300
	No Func.Only Eject/load, Head Drum Running Continuously.
	Check Faulty Unload Or After load Switch. Sw01 And Sw02 On The Deck.

	SHARP
	VC7300
	No Power Indication, No Clock Fuse F902 O/c.
	Change Q908 With 2sc1826 Q920 10 Mfd 50v Q942 10 Mfd 16v

	SHARP
	VC7300
	No Power No Clock
	Q908 2sc1212 C916 10µf

	SHARP
	VC7300
	No Power, No Clock.
	Q908 (2sc1212) Also Replace C916 (10 Uf).

	SHARP
	VC7300
	No Power. Clock Inoperative.
	Replaced Q908, C920 And C942.

	SHARP
	VC7300
	No Servo Lock In Play
	X502 Rcrsa0011 Or Ic504 An6342

	SHARP
	VC7300
	No Servo Lock On Play.
	X502 (rcrsa0011) Or I504 (an6342n).

	SHARP
	VC7300
	Picture Rolling On E-e And Record.
	Check I.F. Package Cct's Output If Ok Check C438 (47 Mfd) Gone Low.

	SHARP
	VC7300
	Poor Or No Colour When Tapes Rec. On Other Mach. Own Rec Ok
	Fit A 270pfd In Parallel With C540 And Fit 1.8 Kohm In Parallel With R522 Then Check Chroma Oscillator Frequency.

	SHARP
	VC7300
	Suddenly Turns Off.Play/rec. Restores Normal Functions.
	Check Take-up Spool Is Stopping. If It Is, Check The Play Idler May Need Replacement. If The Spool Doesn't Stop, The Cassette Lamp Could Just Be Responsible (intermittently O/c) Or Take-up Rotation Sensor Opocoupler Assembly Is Faulty.

	SHARP
	VC7300
	Tangles Or Chews Tapes When Ejected. Prevalent After Rew.
	Replaced Load Belt.

	SHARP
	VC7300
	Tape Looping After Rewind.
	Replace T/u Turntable, Main Brake And Idlers And Check Main Brake Torque As Per Service Manual.

	SHARP
	VC7300
	Tape Wont Load. Head Drum Rotates When Play Is Selected.
	Put Loading Ring Assy In Correct Position And Sequence.

	SHARP
	VC7300
	Won't Accept Or Inject Cassette.
	Check Q8811 Or D313.

	SHARP
	VC7300
	Won't Accept Tape.
	Switch On Front Loading Mechanism Pt No: Qswt0001gezz.

	SHARP
	VC7300
	Wont Accept Tapes
	Switch On Front Loading Mech P# Qswt0001gezz

	SHARP
	VC7700
	Cassette Loading Motor On At All Times.
	Check Q8811 2sd687

	SHARP
	VC7700
	Chopper Tranformer Squealing
	Change C920 (10mfd 50v)

	SHARP
	VC7700
	Dew Sensor Problems.
	Check Q805 And Q806, 2sc1815.

	SHARP
	VC7700
	Drum Rotates At All Times, No Inject Or Eject.
	Check Mechanical Loading Ring Position.

	SHARP
	VC7700
	Int Ejects Tapes, Flap Opening Int. Without A Tape In.
	555 Timer Ics On Mechanon Board Faulty.

	SHARP
	VC7700
	Int Recording.
	Check Ic1301 Pin 8 For Int Loss Opf Signals.

	SHARP
	VC7700
	Laces Up Then Unlaces.
	Change Slack Sensor On Pinch Roller Bracket.

	SHARP
	VC7700
	Loading Motor Weak.
	Change Q8091.

	SHARP
	VC7700
	Loading Motor Won't Rotate.
	Look For Thermal Output To Main Solenoid O/c.

	SHARP
	VC7700
	Loss Of Colour On Pre-rec. Playback Of Own Rec. Ok.
	Fit 270 Pf In Parrallel With C540. Fit 1.8k Ohms 1/4w In Parallel With R522.

	SHARP
	VC7700
	No 12v At T.P. 901.
	On Vc7300 Check R903 0.27 Ohms. On Vc7700 Check R912 0.27 Ohms Q904 2sd1128.

	SHARP
	VC7700
	No Capstan Motor Drive.
	Check Q809, 2sd687.

	SHARP
	VC7700
	No Play F.F. Rew. Or Rec.
	Replaced Capstan Motor.

	SHARP
	VC7700
	No Power Indication, No Clock Fuse F902 O/c.
	Change Q908 With 2sc1826 Q920 10 Mfd 50v Q942 10 Mfd 16v

	SHARP
	VC7700
	Refer Vc7300
	 

	SHARP
	VC7700
	See Vc7300
	 

	SHARP
	VC7700
	Tangles Or Chews When Ejected. Prevalent After Rew.
	Replaced Load Belt.

	SHARP
	VC7700
	Won't Accept Or Inject Cassette.
	Check Q8811 Or D313.

	SHARP
	VC7700
	Won't Turn Off. Cass. Lamp On,head Drum Rotates.
	Check Failure Of Unload End Switch Sw 1. If The Tape Guides Have Not Retracted Fully, Check The Loading Mechanics Starting With The Loading Motor Belt.

	SHARP
	VC7750
	Cassette Loading Motor On At All Times.
	Check Q8811 2sd687

	SHARP
	VC7750
	Chopper Transformer Squealing
	Change C920 (10mfd 50v)

	SHARP
	VC7750
	Dew Sensor Problems.
	Check Q805 And Q806, 2sc1815.

	SHARP
	VC7750
	Drum Rotates At All Times, No Inject Or Eject.
	Check Mechanical Loading Ring Position.

	SHARP
	VC7750
	Int Recording.
	Check Ic1301 Pin 8 For Int Loss Opf Signals.

	SHARP
	VC7750
	Loading Motor Weak.
	Change Q8091.

	SHARP
	VC7750
	Loading Motor Won't Rotate.
	Look For Thermal Output To Main Solenoid O/c.

	SHARP
	VC7750
	Loss Of Colour On Pre-rec. Playback Of Own Rec. Ok.
	Fit 270 Pf In Parrallel With C540. Fit 1.8k Ohms 1/4w In Parallel With R522.

	SHARP
	VC7750
	No 12v At T.P. 901.
	On Vc7300 Check R903 0.27 Ohms. On Vc7700 Check R912 0.27 Ohms Q904 2sd1128.

	SHARP
	VC7750
	No Capstan Motor Drive.
	Check Q809, 2sd687.

	SHARP
	VC7750
	No Power Indication, No Clock Fuse F902 O/c.
	Change Q908 With 2sc1826 Q920 10 Mfd 50v Q942 10 Mfd 16v

	SHARP
	VC7750
	Refer Vc7300
	 

	SHARP
	VC7750
	See Vc7300
	 

	SHARP
	VC7750
	Won't Accept Or Inject Cassette.
	Check Q8811 Or D313.

	SHARP
	VC781
	Int Stops In Rew/ff.
	Earth Cassette Slider By Fitting Spring (mspro113gefj)

	SHARP
	VC782
	Fails Recording After Pause.
	Replace Load Belt.

	SHARP
	VC782
	Hum On Ee Audio.
	Ic601 In Audio Board

	SHARP
	VC782
	Supply Guide Comes Back And Gets Caught On Back Tension Arm.
	Replace Loading Gear Under Supply Guide

	SHARP
	VC787
	Operate Light Goes Out After 8 Seconds
	Check F902 Ur15v Rail

	SHARP
	VC8300
	Agc On Monitor Only Ok In Playback.
	Q1507 No Base Voltage Due To R1540 Being O/c Or High.

	SHARP
	VC8300
	Agc Or Negative Picture.
	Fl4401 S/c.

	SHARP
	VC8300
	Blowing Fuse F803. Wont Accept Or Eject Tape.
	Replace Eject Motor.

	SHARP
	VC8300
	Cap. Speed Varying. Wow In Sound. Servo Phase Signal Faulty
	Remove Bridge 1704 On P.W.B.-a. Change It With 680k Ohms And O.O22 Mfd In Parallel.

	SHARP
	VC8300
	Capstan Running Fast.
	Q718, Q719 S/c.

	SHARP
	VC8300
	Capstan Slows When Hot Noise Band In Pb
	C729 10µf

	SHARP
	VC8300
	Capstan Slows When Hot, Noise Band Thru Picture.
	C729 (1ouf Tan).

	SHARP
	VC8300
	Capstan Speed Varies, Wow In Sound.
	Check Bridge I704 On Pwb A.

	SHARP
	VC8300
	Capstan Varies Speed Wow In Audio
	Check Bridge I704 On Pwb-a

	SHARP
	VC8300
	Cassette Loads But Not Threading.
	Q714, Q716, Q717 S/c.

	SHARP
	VC8300
	Cassette Will Not Load Or Unload Or Eject.
	1. Check For 25v Present On Loading Motor. 2. Check For Faulty Ry801 Load/unload Switch.

	SHARP
	VC8300
	Cassette Will Not Load.
	Cassette Down Switch S2 Broken.

	SHARP
	VC8300
	Chews Or Tangles Tape When Ejected.
	Replace Rubber Boot On Take Up Brake Arm.

	SHARP
	VC8300
	Drum Fails To Start.
	Drum Motor Int. Rmotp101pgezz.

	SHARP
	VC8300
	Drum Wont Start
	Drum Motor Int P# Rmotp1019gezz

	SHARP
	VC8300
	Ejects After Loading Up.
	Change Loading Belt.

	SHARP
	VC8300
	Horizontal Noise Bars.
	1. Capstan Running Slow - Ic1703 2. Dry Joint Thick-film Cr503. 3. Reset D Lock (r711)

	SHARP
	VC8300
	Int Blows F903 When Unlacing.
	Faulty Drum Motor Or Forward/reversee Switch Int. Shorting. (p.No. Qsw-10002ge).

	SHARP
	VC8300
	Int Colour Or Lum In Record
	Ic301 Sa8063

	SHARP
	VC8300
	Int Loss Of Playback Picture (blank Screen)
	Look For D/j's On Plug/socket Converter Cd On Pwb-c.

	SHARP
	VC8300
	Int Stops In Play After Lace Up
	Main Solenoid Sticking. Lub Or Replace

	SHARP
	VC8300
	Int Stops In Play/record
	Slack Sensor Faulty

	SHARP
	VC8300
	Int Stops On Play After Lace-up.
	Main Solenoid Sticking - Lubricate Or Replace.

	SHARP
	VC8300
	Inter. Blows Fuse F903. Blows When Tape Unthreading.
	Check Faulty Drum Motor. Check Intermittent Short In The Forward/reverse Switch (part No. Qswf0002ge). Mounted Near The Solenoids.

	SHARP
	VC8300
	Interm. Colour Flashing Of Self Rec.
	Replaced Ic301.

	SHARP
	VC8300
	Intermittent Colour Flashing On Playback Of Own Recording.
	Change Ic301 Rec. Amp. Vhisa 8063//-1.

	SHARP
	VC8300
	Intermittently Drum Fails To Start In P/back Or Record.
	Change Int. Drum Rmotp1019gezz.

	SHARP
	VC8300
	Intermittently Stops In Play And Record.
	Slack Sensor Faulty.

	SHARP
	VC8300
	Intermittently Stops On P/back Or Rec. After Lace Up.
	Change Main Solenoid Plunger Rplu0046gezz.

	SHARP
	VC8300
	Lines Across Pict. And Sound Wavering.
	Capstan Motor Faulty.

	SHARP
	VC8300
	Loads Up And Ejects Tape.
	Check For Craks In Connector Panel Below Solenoids (at Front Of Deck).

	SHARP
	VC8300
	Machine Stops In Laced Up Position.
	Solenoid Sticking Need Lubricating.

	SHARP
	VC8300
	No "fast Forward"
	Spring (49) Fallen Off.

	SHARP
	VC8300
	No Audio In Ee
	I1502 Ix0043

	SHARP
	VC8300
	No Capstan Drive
	Q718,q719,q720,q721,q723

	SHARP
	VC8300
	No Capstan Drive.
	Q721 (2sd880) In Capstan Brake.

	SHARP
	VC8300
	No Capstan Lock
	Tracking Pot Or Track To Pot O/c

	SHARP
	VC8300
	No Capstan Lock.
	Tracking Pot Or Pc Board To Pot Open Circuit.

	SHARP
	VC8300
	No Capstan Motor Drive.
	Replace All Q718, Q719, Q720, Q721, Q723.

	SHARP
	VC8300
	No Capstan Motor Drive.
	Check Q718. If Faulty Also Check Q719, Q720 Q723 And D711. Transistor Substitutes: Q714, 715 And Q 718, 719 Were 2sc2021. Use 2sc945aq. Q716 And Q720, 723 Were 2sa933. Use 2sa733 Or 2sa950y.

	SHARP
	VC8300
	No Colour.
	1. Ic1505. 2. Cr501. 3. Check Pin 3 Of Pugcb, Adjust Chroma Current Control On Head Amp.

	SHARP
	VC8300
	No Drum Motor Drive
	Replaced Q714,q715,q716,q717

	SHARP
	VC8300
	No Drum Motor Drive.
	Replace Q714, Q715, Q716, Q717.

	SHARP
	VC8300
	No Drum Motor Drive.
	Check Q714. If Faulty Also Check Q715 And Q716. transistor Substitutes: Q714, 715 And Q718, 719 Were 2sc2021. Use 2sc945aq. Q716 And Q720, 723 Were 2sa933. Use 2sa733 Or 2sa950y.

	SHARP
	VC8300
	No Pic On Record/play.
	L405 Faulty Or Ic1402 (ha11703).

	SHARP
	VC8300
	No Picture In Play/record
	L405 Or Ic1402 Ha11703

	SHARP
	VC8300
	No Picture In Playback.
	Change C439 If Fault Still Present Change Ic402.

	SHARP
	VC8300
	No Sound On E-e
	I1502 (ix0043).

	SHARP
	VC8300
	No Sound On Own Recordings Pre-recorded Tapes Ok.
	Ic601 Faulty.

	SHARP
	VC8300
	Noisy Picture After Playing A Pre-recorded Tape Sev. Times.
	Check Erase Osc If Partly Operating On Playback, If So Ic601 Faulty.

	SHARP
	VC8300
	On Playback Looks Like A Capstan And A Drum Servo Fault.
	Check C731 10 Mfd Tant For Leakage Ic702, Ic703 Etc.

	SHARP
	VC8300
	Overshoot On Black To White Transitions On Own Recordings.
	Check Deviation Level Adjustment.

	SHARP
	VC8300
	Patterning On Ch4 Or Snowy On Ch3 Output Of Rf Converter.
	Faulty Rf Converter.

	SHARP
	VC8300
	Ripple In Sound.
	1. Faulty Capstan Motor. 2. Worn/corrugated Pinch Roller.

	SHARP
	VC8300
	Smeary Picture.
	C4413 Or Video-board Dry Joint.

	SHARP
	VC8300
	Snowy Pic On Tuner And Play.
	Q1201 (2sc2570) In Rf Booster.

	SHARP
	VC8300
	Snowy Picture In All Modes
	Q1201 2sc2570 In Rf Booster

	SHARP
	VC8300
	Snowy Picture On Tuner And/or Playback.
	Q1201 In Rf Booster Unit. Use Toshiba 2sc2753.

	SHARP
	VC8300
	Snowy Picture.
	Q1201 In Modulator S/c.

	SHARP
	VC8300
	Stops Int
	Reel Motor Or/and Q6006 2sd687

	SHARP
	VC8300
	Stops Intermittently.
	Check Reel Motor And Q6006 (2sd687).

	SHARP
	VC8300
	Tangles Tape On Eject.
	Change Brake Rubber On Take-up Side Reel. Pgumm0012gezz.

	SHARP
	VC8300
	Tape Stops In Play
	Pinch Solenoid Not Operating. Check Fuse Under Inslulation On Solenoid

	SHARP
	VC8300
	Tape Stops In Play Mode.
	Pinch Solenoid Not Operating, Check Fuse Under Insulation On Solenoid.

	SHARP
	VC8300
	Tapes Getting Chewed.
	Worn Out Brushes In Reel Motor - Change Reel Motor. intermediate Drive Wheel For Supply And Take Up Spools Seized. Rough Edges On Guide Slots For Intermediate Drive Wheel - Smooth Off Roughness Very Carefully Without Enlarging Slots. This Fault Usually

	SHARP
	VC8300
	Tapes Tangle On Eject
	Replace Brke Rubber On T/u Reel

	SHARP
	VC8300
	Tapes Tangle On Eject.
	Replace Brake Rubber On T/u Reel.

	SHARP
	VC8300
	To Operate Mechanism With Top Servo Pcb Up.
	Remove Plug Ao On Servo Pcb.

	SHARP
	VC8300
	Tracking Drifting Over A Couple Of Weeks.
	Change Capstan Motor.

	SHARP
	VC8300
	Will Not Eject From Carriage,wont Allow Carr.To Drop Correc
	Check Lock Off Lever (for Releasing Cassette Flap Broken), Or Has Been Forced Out Of Position. Change Lock Off Lever.

	SHARP
	VC8300
	Will Not Rewind
	Gear Fallen Off Vs Reel-motor.

	SHARP
	VC8300
	Won't Load Or Unload.
	Change Loading Motor Ic1805 Sta401 Motor Changeover Switch (p.No. Qsw-10002ge).

	SHARP
	VC8300
	Won't Play "c" Size Cassette Adaptor.
	Adjust Slack Sensor (vr844) On On Pwb-a.

	SHARP
	VC8300
	Won't Switch Off.
	Check Q902 S/c.

	SHARP
	VC8300
	Wont Play Vhsc Tape In Adaptor
	Adjust Slack Sensor Vr844 On Pwb-a

	SHARP
	VC8300
	Wont Tune To Stations.
	Check Aux/tuner Switch Faulty.

	SHARP
	VC8300
	Wow And Flutter. No Capstan Servo.
	Check Bridge On Pwb A And Or Replace With Original Part.

	SHARP
	VC8300
	Wow In Audio
	Capstan Belt Or Dry Bearings

	SHARP
	VC8300
	Wow In Sound.
	Capstan Belt, Or Dry Bearings In Motor.

	SHARP
	VC8300
	Z Paid
	 

	SHARP
	VC8452
	No Or Intermittent Reel Drive In All Modes.
	Change Ic705, (ta7267p)

	SHARP
	VC8482
	No High Band On Tuner.
	R958 (2.7k0 In Psu.

	SHARP
	VC8482
	No High Band Tunner
	R958 2.7k In Psu

	SHARP
	VC8482
	No Picture In Cue/rewind
	Ic704 Td62104

	SHARP
	VC8482
	No/int Reel Drive
	Ic705 Ta7647

	SHARP
	VC8482
	Won't Accept Cassette.
	Check Operation Of Cass. Down Switch. Pin 1 Of Plug Aa, Cass. Down (l) Should Be (h) With No Cassette In.

	SHARP
	VC8482
	Won't Accept Cassette. Operation Faulty.
	If The Main Cam Gear On The Underside Of Mechanisim Is Wound Fully Clockwise Then Rotate, By Use Of The Loading Motor Worm, 180 Deg Counter Clockwise. A. If Then All Operations Perform Without Faulty Replace Suspect C818, 10µf 16v, On

	SHARP
	VC8581
	Intermittent Recording.
	Check Ic401 (ha11744nt1) Video Processor For Luminance At Pin 20 And Fm Out. Osc Signal At Pin 12 To Video Heads.

	SHARP
	VC9100
	Interm. Chewing, Cuts Off On P/back And Record.
	Check If Reel Idler Ok, Replace Int. Reel Motor. Rmotv1008gezz.

	SHARP
	VC9100
	Interm. White Lines Break Up Of Pic. On E-e And P/back.
	Only On Rf Out Not Video Out. Replace Ic403 On Y/c Pcb.

	SHARP
	VC9100
	Loses Colour On Recordings
	Change Filter Fl504 Rmptdoo52gezz.

	SHARP
	VC9100
	No Picture In Ee Or Playback.
	Replaced Ic403 On Video Pcb.

	SHARP
	VC9100
	No Power, No Clock.
	No 240v To Mains Transformer? Check R901, Change C901 (.1 Mfd). If Voltage To Power Supply Change C9009 (10 Mfd 63v).

	SHARP
	VC9100
	No Reel Motor Voltage.
	Change Q8001 (2sd880).

	SHARP
	VC9100
	No Reel Torque On Playback Or Record.
	Change Q7754 2sd882 And Add 27 Ohm Collector To Emitter.

	SHARP
	VC9100
	No Reg. 12v Pin 2 Ae.
	Check R9019 (15 Ohms). Check Q9006 Use (2sc1826).

	SHARP
	VC9100
	No Video On E-e Mode.
	Change C204 (220mfd 10v).

	SHARP
	VC9100
	Picture Un Stable On Some Channels.
	Replace Zener Ic, 11401, Rhix0037gezz.

	SHARP
	VC9100
	Poor Or No Luminance
	Change Ic403

	SHARP
	VC9100
	Refer Vc9300
	 

	SHARP
	VC9100
	Rf Interf. On Low Ch. Under Weak Signal Conditions.
	Remove R9004 And C9006.

	SHARP
	VC9100
	See Vc9300
	 

	SHARP
	VC9300
	Blows 2.5 A Sb Fuse On Rear Of Vcr
	Q9002 In Psu Or Reel Motor If '02' Type

	SHARP
	VC9300
	Blows 2.5a Sb Fuse At Rear Of Vcr.
	Q9002 In Psu.

	SHARP
	VC9300
	Blows Fuse On P/supply 12v Rail Goes 25v.
	Replace R16 In P/supply And Remove Glue From Pcb.

	SHARP
	VC9300
	Cass. Will Not Eject, Won't Allow Carriage To Drop Corre.
	Check Lock Off Lever (for Releasing Cassette Flap Broken), Or Has Been Forced Out Of Position. Change Lock Off Lever.

	SHARP
	VC9300
	Cassette Will Not Eject.
	Door Flap Not Opening Fully Due To Bent Lever Angle Assembly.

	SHARP
	VC9300
	Chewing Tapes.
	Cassette Down-end (csd) Switch Broken, Or Reel Motor.

	SHARP
	VC9300
	Chews Tapes Int , Stops In Play
	Reel Motor Rmotv1008gezz

	SHARP
	VC9300
	Clock Display Shows Two Days
	Ic5001

	SHARP
	VC9300
	Distorted Or No Pic On E-e.
	Q721 (2sb4568) On Pwb-a.

	SHARP
	VC9300
	Distorted Picture In Ee
	Q721 2sd468 Pwb-a

	SHARP
	VC9300
	Drum Moor On All The Time.
	Remove Glue On Q717 And Q718.

	SHARP
	VC9300
	Drum Speed Int
	X502

	SHARP
	VC9300
	Drum Spins All Time
	Remove Glue On Q717, Q718 Or Q718 Faulty.

	SHARP
	VC9300
	Drum Turns All The Time.
	Q717 (2sc945)

	SHARP
	VC9300
	For Low Reel Torque In All Modes.
	Check For D/j's On Q8001, Located At Rear Of Chassis, By The Head Drum.

	SHARP
	VC9300
	Goes To Stop As Soon As It Is Fully Loaded.
	Ic2002 On Pwc "d". Head Switching Pulses Low In Amplitude.

	SHARP
	VC9300
	Grey Washed Out Pic In Play
	Ic401

	SHARP
	VC9300
	Int Blows 2.5a Fuse At Rear Of Vcr.
	Change Reel Motor If "02" Type.

	SHARP
	VC9300
	Int Capstan Speed
	Ic703

	SHARP
	VC9300
	Int Capstan Speed After 1-2 Hours
	Ic703

	SHARP
	VC9300
	Int Chews Tapes Or Cuts Out In Play/record.
	Reel Motor Int (rmotv1008gezz).

	SHARP
	VC9300
	Int Colour
	Ic503

	SHARP
	VC9300
	Int Colour And Drum Speed
	Ic504

	SHARP
	VC9300
	Int Colour On Recordings.
	Fl504 (doo52ge).

	SHARP
	VC9300
	Int Erratic Behaviour
	Ic801 Cpu

	SHARP
	VC9300
	Int No Power/ Stops
	Q808

	SHARP
	VC9300
	Int Play Or Record.
	Change Idler Assembly And Check For Lazy Drum Motor.

	SHARP
	VC9300
	Int Play Pic
	Fl401

	SHARP
	VC9300
	Int Reel Motor Slows
	R7733

	SHARP
	VC9300
	Int Stops
	C719 Leaky

	SHARP
	VC9300
	Interm. Chewing, Cuts Off On P/back And Record.
	Check If Reel Idler Ok, Replace Int. Reel Motor. Rmotv1008gezz.

	SHARP
	VC9300
	Interm. White Lines Break Up Of Pic. On E-e And P/back.
	Only On Rf Out Not Video Out. Replace Ic403 On Y/c Pcb.

	SHARP
	VC9300
	Intermittent Colour On Playback.
	1. D/j On C534. 2. Cracked P.C. Board Near Centre Retaining Screw Around R538.

	SHARP
	VC9300
	Intermittent No Power.
	D/j Mains I/p Board.

	SHARP
	VC9300
	Intermittent Wow On Sound.
	Change R745. Check Also For D/j's Around Ic7753 And C788 (leaky).

	SHARP
	VC9300
	Intermittently Shuts Down. No Functions No Display
	C903 Low Capacitance. (47uf 16v Servo/sys Con Pcb)

	SHARP
	VC9300
	Loses Colour On Recordings
	Change Filter Fl504 Rmptdoo52gezz.

	SHARP
	VC9300
	Low Reel Motor Torque
	Q7754 2sd882

	SHARP
	VC9300
	Low Reel Motor Torque On Play And Record.
	Q7754 (2sd882).

	SHARP
	VC9300
	Low Reel Torque In All Modes.
	Look For D/j's On Q8001 Located At Rear Of Chassis Along Side Head Drum.

	SHARP
	VC9300
	Mains Fuse Blown (f9001 2.5a)
	Check Q7754 For O/c And R7758 (27 Ohm), Change Q903 And D901 On Mechanon Board.

	SHARP
	VC9300
	No "stop" Function.
	Poor Connection Plug Ha.

	SHARP
	VC9300
	No 12v Reg From Psu
	R9019 15O , Q9006 2sc1983

	SHARP
	VC9300
	No Capstan Drive
	Plug Ad Crimped

	SHARP
	VC9300
	No Colour Int In Record
	Fl504 D0052ge

	SHARP
	VC9300
	No E.E. Picture.
	Check Q721 O/c In Tuner, Use Bc337.

	SHARP
	VC9300
	No Eject
	Ic801

	SHARP
	VC9300
	No Output From Modulator.
	Check L2 O/c (12 Volt Supply).

	SHARP
	VC9300
	No Picture - No Sound.
	Tuner/aux. Switch In Aux./position.

	SHARP
	VC9300
	No Picture In Ee Mode.
	Replaced C204 (220 Mfd 10v).

	SHARP
	VC9300
	No Picture In Ee Or Pb
	Fl202

	SHARP
	VC9300
	No Picture In Ee Or Playback.
	Replaced Ic403 On Video Pcb.

	SHARP
	VC9300
	No Picture In Playback.
	Change C439 If Fault Still Present Change Ic402.

	SHARP
	VC9300
	No Power
	F9001 O/c Q9001 Shorted

	SHARP
	VC9300
	No Power, No Clock.
	No 240v To Mains Transformer? Check R901, Change C901 (.1 Mfd). If Voltage To Power Supply Change C9009 (10 Mfd 63v).

	SHARP
	VC9300
	No Reel Drive
	Q8001 2sd880

	SHARP
	VC9300
	No Reel Drive In Pb/rec But Ff/fr Ok
	Q7754

	SHARP
	VC9300
	No Reel Motor Drive.
	Q8001 (2sd880).

	SHARP
	VC9300
	No Reel Torque On Playback Or Record.
	Change Q7754 2sd882 And Add 27 Ohm Collector To Emitter.

	SHARP
	VC9300
	No Reg 12v From Power Supply.
	R9019 (15 Ohm) Q9006 (2sc1983).

	SHARP
	VC9300
	No Reg. 12v Pin 2 Ae.
	Check R9019 (15 Ohms). Check Q9006 Use (2sc1826).

	SHARP
	VC9300
	No Reverse Search With Tape Inserted.
	Change Reel Motor.

	SHARP
	VC9300
	No Rew., F.F Ok. Pressing Rewind Again Produces F.F. & Rew.
	Check R7751 Relay Sticking.

	SHARP
	VC9300
	No Rewind
	Ry7751

	SHARP
	VC9300
	No Sound. In E.E. And Playback.
	Faulty Rf Converter - Replace.

	SHARP
	VC9300
	No Video On E-e Mode.
	Change C204 (220mfd 10v).

	SHARP
	VC9300
	Noise Bars Floating Through Picture - No Colour On Play.
	X502 (4.43 Mhz) Xtal Faulty. Divided Down For 50 Hz Reference In Capstan Servo, Phase Lock Etc. Can Also Be Failure Of Ic504 (an6342n).

	SHARP
	VC9300
	Noise Bars Move Slowly Through The Pic. Sound Doesn't Wow.
	Check The Capstan Lock Voltage At Tp3 When The Flywheel Is Slowed By Hand, It Doesn't Alter. Usually Waveform Tp1 Is Missing, Due Either To D707 Being Leaky Or R475 (82 K Ohm) O/c. If The Drum And Capstan Servos Are Both Wowing, Check That The Pb 50hz Si

	SHARP
	VC9300
	Noise On Cue
	Lub Roller Asy #17 In Parts List

	SHARP
	VC9300
	Noisy Picture On Own Recording.
	Mono Multi Q702/q703 Out Of Adjustment. Adjust R709.

	SHARP
	VC9300
	Not Erasing On Record
	C611 C512

	SHARP
	VC9300
	On Rec. Noise Bars Floating Through Pic.
	Not Recording Control Pulses On Tape When Recording C717 (.33 Mfd Tant) Faulty. Also Can Be Failure Of I.C. 701 (an6344).

	SHARP
	VC9300
	Pic And Audio Muted On Pause
	Q817

	SHARP
	VC9300
	Pic Unstable In Ee
	Zener I1401 Ix0037ge

	SHARP
	VC9300
	Pic Unstable On E-e
	Zener Ic I1401 (ix0037ge).

	SHARP
	VC9300
	Picture Un Stable On Some Channels.
	Replace Zener Ic, 11401, Rhix0037gezz.

	SHARP
	VC9300
	Plays For Three Sec. Then Motors Stop.
	Int After Load Switch.

	SHARP
	VC9300
	Poor Or No Drum Rotation
	Ic704 M51724p Drum Current Driver

	SHARP
	VC9300
	Poor Or No Luminance
	Change Ic403

	SHARP
	VC9300
	Poor Picture In Ee & Play
	Ic403 Iz0008ge

	SHARP
	VC9300
	Poor Picture No Luminance.
	Replaced Ic403.

	SHARP
	VC9300
	Poor Picture On E-e And Play.
	Ic403 (iz0008ge).

	SHARP
	VC9300
	Poor Recorded Picture.
	C204 (22ouf)

	SHARP
	VC9300
	Recorded Picture Poor
	C204 220 µf

	SHARP
	VC9300
	Rf Interf. On Low Ch. Under Weak Signal Conditions.
	Remove R9004 And C9006.

	SHARP
	VC9300
	Stops After 30 Minutes On Playback
	If Fault Occurs In Play Or Record But Not Fast Wind,check Drum Pick Up Head.

	SHARP
	VC9300
	Stops As Soon As Laced Up
	Ic2002 Pcw-d Head Sw Pulse Low

	SHARP
	VC9300
	Stops For No Reason And /or Chewing Tapes.
	Capstan Bearing Is Binding. Remove, Clean And Lubricate Capstan Flywheel Bearing.

	SHARP
	VC9300
	Tape Jammed.
	Cassette Cover Release Spring (4) Fig. 35 Is Bent - Replace.

	SHARP
	VC9300
	Tape Speed Varies.
	S/h O/p (9) Ic703 Permanently Around 10v. Replace Ic703.

	SHARP
	VC9300
	Tape Spills Out From The Supply Reel: Wont Rew. At End.
	Check Reel Motor Faulty And Will Not Work Under Full Load, Or Reel Idler Wheel Binding On Shaft Or Chassis And/or Clutch Binding, Faulty Slide Switch.

	SHARP
	VC9300
	Tapes Getting Chewed.
	Worn Out Brushes In Reel Motor - Change Reel Motor. intermediate Drive Wheel For Supply And Take Up Spools Seized. Rough Edges On Guide Slots For Intermediate Drive Wheel - Smooth Off Roughness Very Carefully Without Enlarging Slots. This Fault Usually

	SHARP
	VC9300
	The Cassette Housing Stops Half Way.
	Check Eject Finish Switch On The Cassette Housing For O/c.

	SHARP
	VC9300
	Unit Dead.
	1. Fuse F901 Loose - Adjust Holder For Firm Grip Of Fuse. 2. Q9003, Q9002 S/c.

	SHARP
	VC9300
	Very Poor Playback Picture.
	No Signal From One Head, Look For D/j On Rotating Transformer.

	SHARP
	VC9300
	White Out On Ee
	R239 Dj'd

	SHARP
	VC9300
	Won't Play, Rew Or F.F. Record Ok.
	Check Output At Ad4, If So D/j Under Plug Ha13 Or Crack In Cct Board.

	SHARP
	VC9300
	Won't Take Up.
	Remove T/u Spools, Clean And Grease. Replace Idler, Greas Underneath.

	SHARP
	VC9300
	Wont Tune To Stations.
	Check Aux/tuner Switch Faulty.

	SHARP
	VC9500
	Sound Warble.
	Reel Motor Faulty.

	SHARP
	VC9700
	11v And 13v Rails Down.
	Check D9008 In P/s. Also Check For Corrosion Of Component Legs Caused By Holding Glue.

	SHARP
	VC9700
	After Several Hrs Picture Pulling At Top.
	Check For Rubbing Sound From Drum Bearing.

	SHARP
	VC9700
	Chews Tapes.
	Q708 S/c

	SHARP
	VC9700
	Clock Display Too Bright.
	Check D6603 S/c If Clock Ic15002 Faulty. Remove C5007 Before Changing Ic15002.

	SHARP
	VC9700
	Clock Dist./flash. Capstan/drum Motors Interm. Start. -
	Replace Ic5002.

	SHARP
	VC9700
	Display Goes Dim After 1 Hour.
	Check Pr6601 On Audio Board.

	SHARP
	VC9700
	Drum No Go.
	L701 On Servo Pcb Or Remove Glue From Q718 And Q719.

	SHARP
	VC9700
	Failure To Accept Tape.
	Check Cass In Switch If Ok Q810.

	SHARP
	VC9700
	Head Drum To Go.
	Check L701 On Servo Pcb.

	SHARP
	VC9700
	Int Failure To Play.
	Check Drum Doesn't Rotate When Faulty Present, E52 Low 1 Volt. Drum Muting Trans Q719 Leaky.

	SHARP
	VC9700
	Int Failure To Record Sound.
	Change Relays, Change C648 To .1 Mfd, R693 To 10 K Ohm .25w. Or .01.

	SHARP
	VC9700
	Int Loss Of Colour.
	Check Ic301 (sa8063) Overheating. Replace.

	SHARP
	VC9700
	Int Reel Drive.
	Dj On Pin 18 Of Ic704.

	SHARP
	VC9700
	Int Wowing In Play.
	Check Q710 O/c.

	SHARP
	VC9700
	Intermittently Dead With No Clock Display.
	Check Chopper Regulator Chip 19001 (stk722b) Also Q9001.

	SHARP
	VC9700
	Loss Of Field Sync In Record.
	Check C542 On Y/c Board Should Be .1 Mfd Not .33 Mfd.

	SHARP
	VC9700
	No Display
	4O7 Ptc Ht Feed To -30 Volt And Heater Line

	SHARP
	VC9700
	No Go No Clock
	Q5002 Or Circuit Board O/c

	SHARP
	VC9700
	No Line Sync In Visual Search.
	Replace Idler And Reel Motor.

	SHARP
	VC9700
	No Operate, No Clock.
	Q5002 U/s Or Print To Collector O/c.

	SHARP
	VC9700
	No Pic On Play Or E-e Pic Is On Play.
	Glue On Q809 (rec 11v Switch).

	SHARP
	VC9700
	Rf Interference On Low Channels.
	1. Unsolder "mgnd". Green Wire At K9005. 2. Unsolder "gnd" Brown Wire At K9003 And Resolder At C9006 "-".

	SHARP
	VCA101
	Int Stops In Rew/ff.
	Earth Cassette Holder Slider By Fitting Spring (msprp0113gefj).

	SHARP
	VCA101
	Loading Motor Stops Intermittently
	Ic803 Load Motor Driver Ic.

	SHARP
	VCA101
	No Drum Rotation No Drum Afc Apc Ok.
	Replace Ic801 Syscon.

	SHARP
	VCA101
	Not Erasing Audio And Not Recording New Audio
	Hard Wire Full Erase Head

	SHARP
	VCA101
	Shuts Down In Playback Maybe When Warm.
	Check Take Up Hub To Be Stiff Or Seized

	SHARP
	VCA101
	Unit Accepts Tapes Then Ejects Straight Away
	Cassette Detect Switch On Top Of Carriage Is Shorted Closed.

	SHARP
	VCA103
	Hum Bars In Record.
	D906, D907, D908, D909 High Resistance

	SHARP
	VCA103
	Int Stops In Rew/ff
	Hard Wire Full Erasee Head.

	SHARP
	VCA103
	See Vca101
	 

	SHARP
	VCA103
	White Bar Or Distortion Of Tuner Pic. Only Whilst Recording
	Check For Faulty Or Leaky Diode In Power Supply. Check D906, D907, D908 And D909.

	SHARP
	VCA103
	Won't Accept Cass. If No Cass. In Unit Turns Off.
	Check Operation Of Q901, 2sd1565 In Power Circuit.

	SHARP
	VCA103
	Wont Eject Sometimes.
	See Phillips Vr6448

	SHARP
	VCA105
	At Switch On, Loads Then Unloads - Crazy.
	Mode Switch, Clean Contracts, Or Replace.

	SHARP
	VCA105
	Back Tension Arm Jams On Unload
	Replace Plastic Brackets Parts #52 And #53

	SHARP
	VCA105
	Cassette Jams On Eject
	Bend (modify) Pinch Roller Lever Forward 1-1.5 Mil

	SHARP
	VCA105
	Int Rew/ff From Stop Mode
	Replace Idler Ngerh1122gezz

	SHARP
	VCA105
	Laces Up And Then Unlaces No Head Switch
	Fg Pcb Coil O/c On Bottom Of Motor Spike At Contacts Coat With Laquer

	SHARP
	VCA105
	Power Up Erattic Mechanism
	Mode Switch.

	SHARP
	VCA105
	Wont Accept Tape
	Change Sensors Pcb To New Type Duntk3194gezz

	SHARP
	VCA111
	At Switch On, Loads Then Unloads - Crazy.
	Mode Switch, Clean Contacts, Or Replace.

	SHARP
	VCA111
	Back Tension Arm Jams On Unload.
	Plastic Brackets, No: 52 And 53 In Service Manual.

	SHARP
	VCA111
	Cassette Jams On Eject.
	Bend Lever On Pinch Roller Forward 1 - 1.5 Mm.

	SHARP
	VCA111
	Int Rew/ff From Stop Mode.
	Replace Idler. (ngerh1122gezz).

	SHARP
	VCA111
	Laces Up Then Immediatly Unlaces No H.S.P.
	Fg Pcb Coil On Bottom Of Drum Motor O/c. Spike Contracts.

	SHARP
	VCA111
	See Vca105
	 

	SHARP
	VCA111
	Won't Accept Tape.
	Change Sensor Pcb To New Type. Duntk3194he00.

	SHARP
	VCA45
	No Capstan Motor Drive.
	Replaced Leaking Capacitor On Capstan Motor Pcb. check Tracks Haven't Been Destroyed By Leaking Electrolyte.

	SHARP
	VCA502
	All Functions Ok Except Play.No Capstan Drive.
	Capstan Drive Ic X0322ge.

	SHARP
	VCA502
	Eratic Functions When In Rewind,goes F.F.,breaks Tapes.
	Display Stays In Rewind....Replace Capstan Motor.

	SHARP
	VCA502
	Int Stops In Rew/ff.
	Earth Cassette Holder Slider By Fitting Spring (msprp0113gefj).

	SHARP
	VCA502
	Not Erasing Previous Audio Track.
	Hard Wire Full Erase Head.

	SHARP
	VCA502
	See Sharp Vca101
	 

	SHARP
	VCA505
	At Switch On, Loads Then Unloads - Crazy.
	Mode Switch, Clean Contacts.

	SHARP
	VCA505
	Back Tension Arm Jams On Unload.
	Plastic Brackets, Parts 52 And 53 In Manual.

	SHARP
	VCA505
	Cassette Jams On Eject.
	Bend Lever On Pinch Roller Forward 1 - 1.5 Mm.

	SHARP
	VCA505
	Int Rew/ff From Stop Mode.
	Replace Idler Ngerh1122gezz.

	SHARP
	VCA505
	Laces Then Immediately Unlaces. No H.S.P.
	Fg Pcb Coil On Bottom Of Drum Motor O/c. Spike Contracts.

	SHARP
	VCA505
	Screen Green No Audio In Playback.
	No Control Pulse Dirty Heads.

	SHARP
	VCA505
	See Sharp Vca105
	 

	SHARP
	VCA505
	Won't Accept Tape.
	Change Sensor Pcb To New Type Duntk3194he00.

	SHARP
	VCA510
	Cassette Jams On Eject.
	Bend Lever On Pinch Roller Forward 1 - 1.5mm

	SHARP
	VCA510
	See Sharp Vca105
	 

	SHARP
	VCA62
	No Go After Storm.No Display.
	Transistor Q902 2sc2001 Faulty.

	SHARP
	VCA67
	Does Not Pull Tape Back Into Cassette When Unloading. machine Shuts Down Intermittently
	Back Tension Band Felt Has Come Off. Band Sticking To Reel. replaced Back Tension Band. Vslbndk1008gezz

	SHARP
	VCB60
	See Vcb20 Service Manual
	 

	SHARP
	VCD801
	Int Stops In Rew/ff.
	Earth Cassette Holder Slider By Fitting Spring (msprp-113gefj).

	SHARP
	VCD801
	Not Erase Previous Audio Track.
	Hard Wire Full Erase Head.

	SHARP
	VCD805
	Cassette Jams On Eject.
	Bend Lever On Pinch Roller Forward 1 - 1.5 Mm.

	SHARP
	VCD805
	See Vca101
	 

	SHARP
	VCH83X
	Reel Sensor Has No Pulse And Has 12v Where It Should Not!
	Found Connectors On Bus Board Between Power Supply And Eject To Have Corrosion From Liquid.

	SHARP
	VCH851
	Int Stops In Rew/ff.
	Earth Cassette Holder Slider By Fitting Spring (msprpo113gefj)

	SHARP
	VCH851
	Not Erasing Previous Audio Track.
	Hard Wire Full Erase Head.

	SHARP
	VCH851
	See Vca101
	 

	SHARP
	VCH855
	All Tape Functions Stop After Several Seconds.
	Remove And Clean T.U. Reel Sensor, Mounted On Chassis Pcb.

	SHARP
	VCH87
	Picture O.K. Hi-fi Audio O.K. In P/b And Rec. machine Will Not Play Back Linear Audio.
	Replace Faulty Q6306 Transistor With Bc548(check Pin Conn). q6306 Is Surface Mount And Lives On Audio Sub Board(with The Surface Mount Processor).

	SHARP
	VCP4100
	Capstan Runs All The Time.
	C615 Faulty.

	SHARP
	VCP4100
	Capstan Unlocked.
	Change R239 To 390 Ohm, C239 To 22µf, R237 To 2.2m.

	SHARP
	VCP4100
	Chews Tapes.
	Remove T/u Guide Arm Unit.

	SHARP
	VCP4100
	Colour Flickers.
	X302 Faulty.

	SHARP
	VCP4100
	Colour Patterning, Int Colour.
	Remove Earth From Power Lead.

	SHARP
	VCP4100
	D209 Cooks.
	Loom To Dd Shorted To Earth.

	SHARP
	VCP4100
	Improve Dew Detection.
	Change R608 To 56k.

	SHARP
	VCP4100
	Improve Pg Shift.
	Change R215/216 To 18k. Change Vr201/202 To 33k.

	SHARP
	VCP4100
	Int Colour.
	Upc1536c Faulty.

	SHARP
	VCP4100
	Int Servo Lock.
	X301 Must Use Original Type.

	SHARP
	VCP4100
	Looks Like Heads Faulty.
	C329 Faulty.

	SHARP
	VCP4100
	Looks Like Heads Faulty.
	C306, C301, C3095 Faulty.

	SHARP
	VCP4100
	No Capstan Drive.
	C615 Faulty.

	SHARP
	VCP4100
	No Colour.
	C337, C347 Faulty.

	SHARP
	VCP4100
	No Picture On Play.
	C306 Faulty.

	SHARP
	VCP4100
	Noise Bar Thru Pic Every 3 Minutes.
	C229 Faulty.

	SHARP
	VCP4100
	Patterning On Picture.
	Add Earth To Head Leads, Check Lead Dress To Heads.

	SHARP
	VCP4100
	Pic Goes Off Like Heads When Hot.
	C105, Or Dj On Q206 (headswitch).

	SHARP
	VCP4100
	Pic Noise In Play, As Through In Cue.
	C207 Faulty.

	SHARP
	VCP4100
	Pic Skew In Cue/review.
	Change C3a0 To .22µf.

	SHARP
	VCP4100
	Pic Weak, Horiz Bars.
	C387 Faulty.

	SHARP
	VCP4100
	Picture Beat And Patterning.
	C347 Faulty.

	SHARP
	VCP4100
	Stops After 2 Secs In Play.
	Fit New Reel Sensor. Dont Modify.

	SHARP
	VCP4100
	Tracking Doesn't Adjust.
	C205 Fautly.

	SHARP
	VCP4100
	White Flicker Noise.
	C317, C318 Fautly.

	SHARP
	VCT510
	At Switch On, Loads Then Unloads - Crazy.
	Mode Switch, Clean Contacts.

	SHARP
	VCT510
	Back Tension Arm Jams On Unload.
	Plastic Brackets, Parts 52 And 53 In Manual.

	SHARP
	VCT510
	Laces Then Immediatly Unlaces. No H.S.P.
	Fg Pcb Coil On Bottom Of Drum Motoro/c. Spike Contacts, Coats With Laquer.

	SHARP
	VCT510
	See Sharp Vca105
	 

	SHARP
	VCT510
	Won't Accept Tape.
	Change Sensor Pcb To New Type. Duntk3194he00.

	SHARP
	VLC6100
	Snowy Picture, Sometimes 1/2 Screen
	Replaced Servo Smd Ic. Ir3p71 Lmir3p711 On Main Board

	SHARP
	VLC670
	No Audio In Play Or Record Modes
	Audio Hybrib.?? Lmrhiz0093tazz

	SHARP
	VLC770
	No Power.
	C 802 On Main Syscon Pcb 10µ/16v Smd Cap . Dcdc Converter And Audio Hybrib

	SHARP
	VLC8000
	Ghosting In Playback
	Unit Needs To Be Recapped. c2206 47 µ6v Near Connector Bc On Y/c Pcb

	SHARP
	VLM78E
	No Colour From Recorded Tape, Pb Ok
	10 µ Caps C420. Also 480,411,416. 22 µ Appeared To Be Ok, But Was Replaced.

	SHARP
	VLM78E
	See Sharp Vlm4x Similar
	 

	SHARP
	VLM78E
	See Vlm4x
	Similar To Vlm4x

	SHARP
	XC30
	No Video
	Check If Nothing At Tp3. Check Q102 Collector Volts Low (18v). Target Connector To Screening Shield S/c.
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