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Many More Tips In Ours Members Section!
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11

[image: image73.jpg]



[image: image74.jpg]



[image: image75.jpg]



To Remove Limitations, Click HERE!
[image: image76.jpg]



[image: image77.jpg]



[image: image78.jpg]



PLEASE CHOOSE A BRAND:
Top of Form

[image: image79.wmf]

Select Brand


Bottom of Form

[image: image80.jpg]



[image: image81.jpg]



[image: image82.jpg]



Our Store!












































SHARP 
SHARP
GENERAL
Drum Won't Spin
Rubber "o"ring Loose Inside Remove Head Drum Assy And Remove .....Don't Force....
SHARP
VC200
Mode Cogs Go Out Of Alignment.
Pin Missing In Brake Slide.
SHARP
VC2300
Drum Rotates Very Fast At All Times Operate Is On.
Suspect Ic706, M51724p, On Servo Pcb.
SHARP
VC2300
Machine Dead With Tape In Laced Up Position.
Check Q914 (2sa770) On Servo Board O/c.
SHARP
VC2300
No Capstan Drive
L701 O/c Servo Pcb Rtrnz0012gezz
SHARP
VC2300
No Capstan Drive.
L701 O/c On Servo Pcb. Pt No: Rtnz0012gezz.
SHARP
VC2300
No Power Ac Adaptor Fails
Q3 Q4 2sc2826
SHARP
VC2300
No Power, Ac Adaptor Fails.
Q3 And Q4. 2sc2826 Use Original Parts.
SHARP
VC2300
Pause, Stop & Record Leds All Lit. With No Deck Functions.
Check Ic807 By Replacement. Check Loading Motor Chip Ic808 And Loading Motor Should Draw 100ma.
SHARP
VC2300
Problems With Rewind
Change Reel Motor.
SHARP
VC2300
Sound Fluctuating
Check Capstan Motor Faulty.
SHARP
VC330
Poor Wind And Rewind Playback Ok.
Check Aux. Brake Not Releasing Because Ic901 Faulty.
SHARP
VC330
Reel And Capstan Motors Going Backwards.
Change Ic711
SHARP
VC3300
No Channel Indicator, No Go.
No 12v At Tp901. Check Q904, Q902, Q903, On Pwb-p.
SHARP
VC3300
No Tuner Function And Channel Indicators Not Functioning.
Replaced Transistor Q904 And C903 On Pwb-p.
SHARP
VC3300
Reel Motor Too Fast Causing Tape Speed To Increase.
Q863 Shorted, Also Replace Reel Motor If "02" Type.
SHARP
VC3300
Tuner Faulty, Wont Tune In Stations.
Check For 31.5v On Pin 5 Of Plug Ic. If Faulty Check Function Of Zener Ic201, Ix0037ce, On Pwb-1.
SHARP
VC3300
Won't Tune Stations.
Ic201 (31v Zener) Rhix0037cezz.
SHARP
VC381
Audio Low Volume.
Change D606 Leaky Is119.
SHARP
VC381
Cassette Door Opens Only Half Way On Eject.
Lid Lever Angle Assembly Bent. Rebend To Work.
SHARP
VC381
Clock Will Not Reset.
Change Mp2812 Under Display Panel.
SHARP
VC381
Dew Sensor Problems
Change R801 47k Ohms With 470k
SHARP
VC381
Drum Servo Faulty On Record
Q702,q703 Buffer Osl 2sa945
SHARP
VC381
F901 Or F902 Blows, Int Failure To Rewind Int Tape Spillage
Check Worn Idler If Ok Reel Motor Suspect.
SHARP
VC381
Intermittent Or No Eject.
Ic803 (m54532p)
SHARP
VC381
Intermittently Stopping On Play Or Rec., Chewing Tapes.
Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).
SHARP
VC381
Low Audio
D606 Leaky Iss119
SHARP
VC381
No Capstan Drive In Record Mode.
D612 On Audio Board Pwb-b Measures Ok But Is Leaky. Is119.
SHARP
VC381
No Chroma In Rec Or Pb
Fl501 Rmptd0131gezz
SHARP
VC381
No Colour On Play Or Record.
Fl501 (rmptdo131gezz). Also Check Fl503
SHARP
VC381
No Eject.
Change Ic803 (vhim54532p/-1)
SHARP
VC381
No Functions 4 Amp Fuse Blown.
Check 12 Volt Supply If High (18v) Reg Transistor S/c. make Sure Replacement Is Mounted Correctly On Heatsink (original Is Not).
SHARP
VC381
No Go - 2.5 Amp. Powerfuse Blown.
Check/ Replace Reel Motor - Always Change Reel Motors With Type Numbers Ending In 02.
SHARP
VC381
No Replay Audio Ee Audio Ok
C621 S/cct (100uf 25v)
SHARP
VC381
No Video On E-r Mode.
Check Ic309 For O/c - Or C206 For S/c.
SHARP
VC381
No Video On Playback
Change Ic308.
SHARP
VC381
Not Erasing Previous Audio Track.
Audio Cable Shorted Under Plastic Tie Near Audio/ctl Head.
SHARP
VC381
Picture Rolling On E-e And Record.
Change C438 47 Mfd, C439 (nearly O/c). If Ok Check Around Ic201 And Ic402.
SHARP
VC381
Playback In Colour Will Not Record In Colour.
Check Fl503. The Down Converted Signal Should Be 500 millivolt P-p On Pin 1 Of Colour I.C. The Carrier Signal Should Be 500 Millivolt P-p At Pin 28.
SHARP
VC381
Remote Erratic.
C811 (.01 Uf) Leaky.
SHARP
VC381
When Play Is Selected Squeaking From Head Drum, Then Stops.
Change Reel Idler
SHARP
VC381
When Record Is Selected Machine Fails To Stay In Record.
Check T/u Reel Not Turning In Record Mode. Playback Ok. Change Ic7754.
SHARP
VC381
When Replacing Cass Lamp, To Check Correct One Is Fitted. .
Check Voltage R872-5. Check Voltage On Point Where Ic802 And R872-5 Connect, Should Be 8 Volts If Lower Wrong Cass Bulb Has Been Used.
SHARP
VC381
Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.
SHARP
VC381X
No Record Colour.
Replaced Filter Fl503.
SHARP
VC381X
Take Up Spool Not Rotating In Record. Ok In Playback.
Change Ic7754.
SHARP
VC381X
When Pic. Search Is Selec. Mach. F/f Or Rew.
Check For 9.9v On Pin 32 Of Ic801. Change Ic801, D7758 If Still Present Check Ic805 And Ic806 If Ok Check Pins 1,4,5 Of 17754 Go High In Search Mode And Pins 12, 13, 16 Go Low. If D7753 Cathode Is Not High At This Time, Change Q7751 If Pin 59 Of Ic801 Do
SHARP
VC383
Intermittently Stopping On Play Or Rec., Chewing Tapes.
Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).
SHARP
VC383
Low T/u Torque.
Adjust R7765 "tu Torque".
SHARP
VC383
No Video On E-r Mode.
Check Ic309 For O/c - Or C206 For S/c.
SHARP
VC383
No Video On Playback
Change Ic308.
SHARP
VC383
Refer Vc381
SHARP
VC383
Self Rec. Tapes, Band Few Lines Deep,third Way Down.
Check Record Switching Monostable Faulty, Check C714 And Reel Motor And Idler.
SHARP
VC383
Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.
SHARP
VC386
Audio Click In P/back. Usually Only 1 Channel.
Rh-1z0038ge. Need Switch Ic Audio.
SHARP
VC386
Audio Low On One Channel
Replace Ic651 Rh1z0038gezz
SHARP
VC386
Audio Low On One Channel Of Own Record.
Change Ic Rh120038gezz.
SHARP
VC386
Audio Low On One Channel.
Replace Ic651 (rh1z0038gezz).
SHARP
VC386
Blank Screen On Play And Tuner.
L 409 (220 Uh) On Video Pcb.
SHARP
VC386
Blank Screen On Play Or E-e.
No 12v On Pin5 Of Ic402. Check L407, L409 On Video Pcb.
SHARP
VC386
Capstan Fails To Start
D6605
SHARP
VC386
Clock Flashes & Returns To Ch1, As If Power Was Interrupted
Replace All Electro's In Psu.
SHARP
VC386
Clock Flashes And Resets To Ch1 As If Lost Power
Replace All Electros In Psu, Specifically C16 (10uf 50v)
SHARP
VC386
Drum Rotating Too Fast.
Chek C710 S/c.
SHARP
VC386
Flickering Colour
Fl503 Rmptd0052gezz
SHARP
VC386
Flickering Colour.
Fl503 (rmptd0052gezz).
SHARP
VC386
Flickering Colour.
Change Filter Fl503. Rmpdt0052gezz.
SHARP
VC386
Int No Function Of Channel Change.
Check For D/j On Socket Ta On Pwb.
SHARP
VC386
Interm. Colour In P/back Or Rec. No Colour In P/back Rec.
Replace Fl503.
SHARP
VC386
Intermittently Stopping On Play Or Rec., Chewing Tapes.
Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).
SHARP
VC386
Low Sound
Q6601 (bc337) Pin 3 Bi 8.5 Volts.
SHARP
VC386
No Colour In Record
Ic501 Ha11781nt, Fl503 Rmptd0052gezz
SHARP
VC386
No Colour On Record.
Ic501 (ha11781nt) Or Fl503 (rmptdoo52gezz)
SHARP
VC386
No Picture In Pb Or Ee
L409 220µh ,l407 On Video Pcb.Check 12v Pin 5 Ic402
SHARP
VC386
No Power And Audio Pcb
Check C/protector On M/board Near Tracking Control (12v)
SHARP
VC386
No Video On E-r Mode.
Check Ic309 For O/c - Or C206 For S/c.
SHARP
VC386
No Video On Playback
Change Ic308.
SHARP
VC386
Poor Colour Saturation On Still Of Pre-recorded Tapes.
Change R429 To 1k Ohm On Y/c Pcb.
SHARP
VC386
Traking Control No Effect.
Tracking Control O/c.
SHARP
VC386
Tuning Drift All Channels.
Check D1430 On Tuning Board Leaky. Also D1425 - 1444.
SHARP
VC386
Tuning Drift.
Check Pr01 Regulator Also Ic1403 Or Int Tuning Pots.
SHARP
VC386
Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.
SHARP
VC386..
No/int Reel Drive.
Ic705 Ta7267p.
SHARP
VC387
Faulty Audio
Protector Ic619 On Audio Pcb O/c Icp-n10
SHARP
VC387
Faulty Audio.
Protector Ic619 On Audio Pcb O/c. Icp-n10.
SHARP
VC387
Intermittently Stopping On Play Or Rec., Chewing Tapes.
Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).
SHARP
VC387
No Drum Rotation.
14 Volt Supply Fuse O/c Not Shown On Cct.
SHARP
VC387
No Power On, Clock Ok.
Check For 9 Volt On Pin 64 Of Ic801, If Not, Look For O/c Semiconductor Fuse Not Shown On Cct.
SHARP
VC387
No Tuner, Blank Screen.
Check R954 (2.2 Ohm) And Check Q953, Q954, And Electro's In Psu.
SHARP
VC387
No Tuner. Blank Screen
Check R954 2.2 O Q953 Q956, Q955 & Electros In Psu
SHARP
VC387
No Video On E-r Mode.
Check Ic309 For O/c - Or C206 For S/c.
SHARP
VC387
No Video On Playback
Change Ic308.
SHARP
VC387
Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.
SHARP
VC387
Won't Operate.
Protector Ic815 On Mecha Cont Pcb. Icp-n5.
SHARP
VC387
Wont Operate
Proctector Ic815 Icpn10 Mecha Pcb
SHARP
VC388
Intermittently Stopping On Play Or Rec., Chewing Tapes.
Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).
SHARP
VC388
No Colour In Play
Replace X502 4.433 Mhz Adjust
SHARP
VC388
No Colour On Play.
Replace 4.433 Xtal. (x502) - Adjust Frequency.
SHARP
VC388
No Functions.
Check Q5002 S/c Because Ic15002 S/c.
SHARP
VC388
No Go
Q1 2sc2625, Ic1 Pc511n
SHARP
VC388
No Power. No Clock. No Functions
Q5002 O/c No +5v Rail. Aprox Load Current 90-100 Ma
SHARP
VC388
No Video On E-r Mode.
Check Ic309 For O/c - Or C206 For S/c.
SHARP
VC388
No Video On Playback
Change Ic308.
SHARP
VC388
Power No Go.
Q1 (2sc2625) And Ic1 (pc511n).
SHARP
VC388
Power Supply Faulty After Fitting A New Capstan Motor.
Check: Q1 (2sc2625) Chopper Ic1 Pc511n. Also Change C7022 To (1 Mfd 50v) R7040 To (27k Ohms)
SHARP
VC388
Power Supply Wont Start Reliably
Reduce Value Of R32/r57 To 27r Instead Of 54r
SHARP
VC388
Snowy Or Flyscreen Effect On Own Recording.
Reduce Chroma Record Current.
SHARP
VC388
Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.
SHARP
VC388
Won't Load Tape.
I 806 (s16900a).
SHARP
VC388
Wont Load
Ic806 Si6900a
SHARP
VC390
Black Streaks In Playback
Heads Ok, Check 3.8 Mhz Oscillator Is Not Running At 5 Mhz.. C227 Intermittent Replace. Readjusting Will Not Repair The Fault
SHARP
VC390
Int Wont Record Picture
Q204, Q205 2sa733
SHARP
VC390
Intermittently Stopping On Play Or Rec., Chewing Tapes.
Change Reel Idler Or Reel Motor (commonly Intermittent In Operation).
SHARP
VC390
Locked In Lp Or Sp Frontpanel Ctrl Won't Affect.
Check Sw8001 And Sw8002 Are Inthe Mid Position.
SHARP
VC390
Looks Like Video Heads, Black Streaky Lines In Playback
Replacing Heads Didnt Fix . The Problem Was The 3.8 Mhz Fm Oscillator Was Running Naer 5mhz. Trimmer Cap C227 Intermittent. Readjusting It Worked, But It Has To Be Replaced. to Adjust The Free-run Freq, Put Vcr In Line In Mode And Place A Frequency Coun
SHARP
VC390
No Picture In Play
Ic308 Protector Icp N10
SHARP
VC390
No Video On E-e Mode.
Check Ic309 For O/c - Or C206 For S/c.
SHARP
VC390
No Video On Playback.
Change Ic308.
SHARP
VC390
Poor Record Looks Like Stuffed Heads.
C227 Possibly Faulty( Fm Freq) Adjust And Return To Previous Setting To Check.
SHARP
VC390
Poor Recording
Ry301 Contacts Dirty - Clean And Replace.
SHARP
VC390
Shuts Down After 30 Mins.
Replace C12 In Power Supply 220uf 16v
SHARP
VC390
White Lines/dots In Play
C17 220µf/16v In Psu
SHARP
VC390
Will Inject And Eject Tapes Ok, Tuner Ok, No Functions.
Check Cass Lamp, Should Be On At All Times. If Not, Check Cass Down Switch Bent Or Faulty, Repair Or Replace.
SHARP
VC390
Will Not Eject Tape.
Check Lever On Rhs Of Eject Mechanism Activates Micro Switch Clean And Service.
SHARP
VC468
Int Picture Rolling On Playback.
Check R743 Has No Effect If So C725 Gone O/c.
SHARP
VC481
Capstan Fails To Start
Mode Switch
SHARP
VC481
Capstan Fails To Start.
Mode Switch. Qsw-r0010gezz.
SHARP
VC481
Capstan Slow In Play/rec
D742 Servo Pcb
SHARP
VC481
Capstan Slow In Play/rec.
D742 On Servo Pcb.
SHARP
VC481
Capstan Unlocked.
Check Tracking Control For Dry Joints.
SHARP
VC481
Capstan Won't Lock Even After Replacing, Motor, Bearing, And Doing A Lock Adjustment.
Check For Spikes On Control Track Signal. If So Replace Capstan Servo Chip(ic702)
SHARP
VC481
Cassette Inject Faulty.
Won't Open Door Of Cassette. Change Slider Assembly. Lhldx3016gezz.
SHARP
VC481
Chews Tapes No Rewind
Q8022 Phot Transistor Px0053gezz
SHARP
VC481
Chews Tapes, No Rewind.
D734 Leaky, Off Pin 10 Of Ic 708 On Pwb-a.
SHARP
VC481
Goes Into Rewind.
Q8022 Photo Transistor. Px0053gezz.
SHARP
VC481
Interm Reel Motor Drive.
Check For Dry Joints On Q713.
SHARP
VC481
Interm. Capstan Motor Drive.
Check For Dry Joints On Q708.
SHARP
VC481
No Capstan Lock.
R794 (4.7k). Put Another 4.7k In Parallel. On Capstan Servo Pcb
SHARP
VC481
No Or Flickering E-e Pic. In Stop Mode Pb. 9v Is 3v S/b 0v.
Ic802 (ir2403 Or Td62105) Faulty.
SHARP
VC481
No Reel Drive
Ic708 Faulty Placing 3v Dc On Reel Drive Switch Input (ic705,p2)
SHARP
VC481
Operation Light Not On.
Change Protector Pr801 Qfs - P1021gezz. Change Q813 2sc945 On Mechanon Board Pwb-e. C452 S/c On Y/c Board, Also Check Pr-eb Protector On Pwb-e.
SHARP
VC481
Picture Flickering In Ee
Pb9v Rail Is 3volts. Ic802 Ir2403/td62105
SHARP
VC481
Won't Accept Tape.
Slider Assy. Lhldx3016gezz.
SHARP
VC481
Won't Accept Tape.
Cassette Switch On Cassette Carriage O/c. Qsw-f0010gezz.
SHARP
VC481
Won't Tune Stations.
Ic951 On Power Supply Pcb.
SHARP
VC481
Wont Accept Tapes
Carrige Switches Qsw F0010gezz
SHARP
VC481
Wont Accept Tapes
Slider Asy Lhldx3016gezz
SHARP
VC481
Wont Tune Channels
Ic951 In Psu
SHARP
VC482
Play Selec. Goes Into F.F Search. Own Rec. Ok On Other Mach
Check Pin 5 Of Ic802, If Not Zero Volts Change Ic802.
SHARP
VC482
Refer Vc481.
SHARP
VC482
See Sharp Vc481
SHARP
VC482
Wont Record Or Erase Sound.
Check If Q603 (2sc2001) Leaky.
SHARP
VC483
Power Supply O.K. But No Display Or Functions.
Pr801 Fuseable Resistor Faulty.
SHARP
VC483
See Sharp Vc481
SHARP
VC483
Tape Counter Not Working
Check For Obstructions To Auxiliary Pulse Generator Wheel.
SHARP
VC486
Clock Gains 10mins/day. C5007 Wont Adjust Tp2 To 131.072khz
C5006 (10pf) In Parallel With Trimmer O/c.
SHARP
VC486
Clock Runs Fast
Adjust Tp2 For 131.072khz If Not C5006 O/c
SHARP
VC486
Counter Erratic
Photo Sensors Faulty Or Need Clean
SHARP
VC486
Counter Numbers Erratic.
Q8004 And Q8005 Photo Interrupters Faulty.
SHARP
VC486
Counter Problems.
Change 2x Photo Interrupters.
SHARP
VC486
Cyclic Noise Bar On Play
Check C743 100uf 16v Cap. (bias Bypass For Control Track Pulse Amp.
SHARP
VC486
Erratic Behaviour Of Deck.
Check Faulty Mode Switch.
SHARP
VC486
Faulty Load/unload In P/back & Rec. Interm.Changes Mode.
Change Mechanism Position Switch. Qsw-r0008gezz.
SHARP
VC486
Goes To Stop Just As It Fully Loads.
Drum Pg Coil O/c. On Lower Drum Under Rotary Tx.
SHARP
VC486
Int Changes Mode, Chews Tapes
Mode Switch Qsw R0008gezz
SHARP
VC486
Int Changes Mode, Chews.
Mode Switch. Qsw-r0008gezz.
SHARP
VC486
Int Cuts Out In Pb
Replace Reel Sensors
SHARP
VC486
Int Cuts Out In Play/record After 1 Hour.
Replace Reel Sensors.
SHARP
VC486
Int Picture Rolling On Playback.
Check C725 On Servo Board.
SHARP
VC486
Interm. Cuts Off On P/back Or Rec After I Hour Approx.
Change Reel Sensors - Photo Interrupters Rh-px0042gezz.
SHARP
VC486
Method Of Adjusting Capstan Servo Lock.
Short Ends Of D763. Adjust R777 To Give 3.6v At Pin 5 Of T.P.B. When Short Is Removed Voltage May Change Though Should Remain Stable.
SHARP
VC486
Mod. To Prev. Overheating Ic714 In Servo Circuit.
On Track Side Of Servo Pcb Place A 100 Ohm .5w And A 10 Mfd 16v Electro In Series From Emitter Of Q717 To Pin 8 Of Ic714.
SHARP
VC486
No Clock, No Functions. Tuning Stuck On Ch O.
X5001 Faulty Or Ceramic Caps On Track Side Of Pcb Causing Shorts.
SHARP
VC486
No Clock, No Go, Wont Change Channels
X5001 Or Cermac Caps Shorting On Pcb Side.
SHARP
VC486
No Colour In Pb Or Rec
Q501 2sc2308
SHARP
VC486
No Colour On Play/record.
Q501 (2sc2308) Faulty.
SHARP
VC486
No Functions.
Capstan Mtr Ic And Micropocessor Ic .Suspect Capstan Mtr.
SHARP
VC486
No Functions.
Microprocessor, Capstan Drive Ic Shorted, Suspect Capstan Motor.
SHARP
VC486
No Load/eject
Ic808 Ta7267
SHARP
VC486
No Reel Drive
Ic810 Ta7267 Q826,q827,q828
SHARP
VC486
No Reel Drive.
Ic810 (ta7267p/-1) And Check Q826, Q827, Q828.
SHARP
VC486
No Reel Motor Drive.
Change Ic810 (ta7267p/-1). Check Q826, Q827, Q828.
SHARP
VC486
No Remote Control.
Check Ic812 (lr3711m/-1). Check Possible Faulty Mode Switch.
SHARP
VC486
Operation Light Not On
See Same Fault Vc481 Above.
SHARP
VC486
Reel Motor Wont Turn When Laced Up And Playing. Tape Stuck
Change Ic715 On Pwb-a Vhiba6209//-1.
SHARP
VC486
Rf Inter. On P/back. Could Be Vcr To Close To Tv Transmitter
1. On Pwb-x Head Amp. Board Cut Tracks On Pins 6 & 8 Of Ic3301. Place A Ferrite Bead Of 4 Turns Across Each Track. 2. Add 180 Pf Capacitors From The Audio In And Out Rca Sockets To Earth. Hardwire Input Board Gnd. To Power Supply Gnd.
SHARP
VC486
Tape Counter Counting Faulty.
1. Check The Lower Reflective Surface On The Counter Relay Pulley On Top Deck Of Mechanism. If The Reflective Surface Is Not Perfect - Replace. P.No. Nplyv0088gezz. 2. Check And Clean Photo Interruptor Sensors. P.No.
SHARP
VC486
Vert Jitter Etc On Own Recordings.
Q711 Heat Sensitive. Head Switching Varies.
SHARP
VC486
Vert Jitter In Self Rec
Q711 Head Switch Varies
SHARP
VC486
Won't Accept Cassette. Operation Faulty.
Refer Same Fault Sharp Vc8482. Replace C826, 10µf 16v, On Mecha Control Pcb.
SHARP
VC486
Won't Record Or Play Colour Intermittently.
Fl505 5.2mhz Filter Faulty.
SHARP
VC486
Wont Load Or Eject Tapes.
Ic808 (ta7267p).
SHARP
VC486
Wont Turn On
C532 Shorted On Pwb-c
SHARP
VC486
Wont Turn On.
Check C532 Shorted On Pwb-c.
SHARP
VC488
Colour Dashes All Over Screen On Play.
Earth Capstan Drive Ic Heatsink, And Add .01uf From Pin 9 To Earth.
SHARP
VC488
Colour Dashes In Pb
Earth Capstan Drive Ic H/sink, Add .01µf B/t Pin 9 & Earth
SHARP
VC488
Goes Into Ff, Rew, Stop Etc By Itself.
Q805 On Pwb-e (2sc174) In Syscon.
SHARP
VC488
Goes To Stop Just As It Fully Loads Up
Drum Pg Coil On Lower Drum O/c (under Rotary Transformer)
SHARP
VC488
Hifi Light Flickers & Goes Out When Hot Or No Hifi On Play.
Audio 9v Goes Low, Ic953 95kucz0072gezz. M5230 L Ic On Power Supply Board, Its A Bitch To Get At
SHARP
VC488
Int Changes Mode, Chews Tapes Etc.
Mode Switch. Qsw-r0008gezz.
SHARP
VC488
Int Goes Into Any Mode By Itself
C805 Syscon 2sc174
SHARP
VC488
Laces Up Then Unlaces, Drum Turns For Sec. Or Pic Shakes.
Drum Motor Rmotp1071gezz.
SHARP
VC488
Lines In Pb. Tracking Not Working
Pots In Drawer O/c Repace
SHARP
VC488
Looks Like Heads Faulty.
Electros In Psu. C956(1uf), C962(1uf), C957(.047uf).
SHARP
VC488
No Audio No Functions
Ic5006 Rhix0014gezz Microproccer
SHARP
VC488
No Capstan Lock, No Ctl.
C776 (100µf/16v).
SHARP
VC488
No Chroma On Play.
Mn6163 Chroma Ic.
SHARP
VC488
No Reel Drive In Any Mode.
Suspect Ic715, Ba6209 On Servo Pcb.
SHARP
VC488
No Sound, No Clock Or Channel Display, Ch Buttons Dont Work
Ic5006 Rhix0014gezz Microprocessor.
SHARP
VC488
Picture Rolls Like Loss Of Capstan Lock. Capstan Servo Adjust Helps But Not Good Enough.
Replace C776(100uf 16v) Electrolytic Capacitor, On Servo Pcb. (top Left Board). It Was Short Circuit.
SHARP
VC488
Picture Shakes Or Wont Play.
Drum Motor Rmotp1071gezz
SHARP
VC488
Reel Wont Turn When Fully Loaded Wont Eject.
Ic715 On Pwb-a. Vhiba6209//-1
SHARP
VC488
See Vc486
SHARP
VC488
Static In Pb. (looks Like Heads)
Electros In Psu C956, C962 , C963 = 1µf & C957 .047µf c956 In Particular
SHARP
VC488
Stopped In Laced Position.
Mode Switch. Qswr0008gezz.
SHARP
VC488
Switches On, Switches Off, Laces Up Weird Problems.
Pcb Behind Timer/clock Display Full Of Dj's Where Leads Connect To Pcb.
SHARP
VC488
Tape Remain Indicator Erratic.
Reflective Stripes On T/u Reel U/s Or Q903 In Psu.
SHARP
VC488
Tracking Bars On Screen
C776 100µf In Control Amp
SHARP
VC488
Traking Not Working.
Check 3 Pots In Drawer, One Or All May Be O/c.
SHARP
VC581
Black Screen In Ee
Cracked Pcb Near Rf Booster
SHARP
VC581
Black Screen On E-e.
Craked Pcb Around Rf Booster.
SHARP
VC581
Buzz In Sound.
Change T1501 Pif.-det. Transformer. New Types 0029.
SHARP
VC581
C/stan Rotates B/wards When Stop Pressed. Stops When Played
Check Shorting Links J20/j25 Shorting Out On R/h Side Of Mother Board.
SHARP
VC581
Capstan On At All Times. No Reel Motor Drive.
Check Operation Of Ic706, Bu4011b.
SHARP
VC581
Capstan Speed Varies On Play And Record.
Replace Ic704. Rh-1x0107gezz.
SHARP
VC581
E-e Picture Distorted.
Ic1501. (x0275ce).
SHARP
VC581
Ee Picture Is Distorted
Ic1501 X0275ce
SHARP
VC581
Functions Faulty, No Motor Drives.
No 14v At Pin 7 Of Plug Pa On Power Supply. Check For Circuit Protector Ip901 In Power Circuit. P.No. 95kpjc285zz.
SHARP
VC581
Goes Into Any Mode As Soon As Operation On.
Change Q812 Vsdta124es/-1. Should Have 4.5v At Pin 43 Of Ic801.
SHARP
VC581
Intermittent Functions.
Q812 (dta124).
SHARP
VC581
Looses Drum And Capstan Lock In Play
Dry Joint On Xtal X501 In Chroma Section
SHARP
VC581
No Colour On Play Or Record.
Fl501 (rmptdo131gezz). Also Check Fl503
SHARP
VC581
No Go Clock Ok
Ip901 2.5 Amp O.C In Psu
SHARP
VC581
No Go, Clock Ok.
Ip901 2.5a O/c In Psu.
SHARP
VC581
No Operate Led
No Pcon 12 V Check Ic902 M5236l
SHARP
VC581
No Operation Light. Laces Up Then Unlaces.
Check Ic902 In Power Supply.
SHARP
VC581
No Reel Drive
Ic702 Ta7267p
SHARP
VC581
No Reel Motor Drive.
Change Ic702, (ta7267p).
SHARP
VC581
No Tape Functions, No Operate Led.
Fuse On Psu, P901 2.5 Amp
SHARP
VC581
Operation Faulty.
Check P.Con. 9v Switch, Q909, 2sc3518 In Power Supply. if Faulty Or Overheating, Check For Short Circuit To Ground On P.Con. 9v Line, Pins 14-15 Of Plug Pa. If Short To Ground, Check For Faulty C219, 100µf 16v, Near The Edge Of Main Pcb, Near Ic 402.
SHARP
VC581
Pause/still Indicator On But Cont. To Play Or Record.
Remove C8001 (47 Mfd 16v) Pwb-w Across Loading Motor.
SHARP
VC581
When Tuning To Station - Goes To Blank Screen Agc Faulty.
Change Ic1501
SHARP
VC581X
Wont Play Or F.F. Supply Brake Stuck On.
Replace Microcomputer Ic801.
SHARP
VC584
Clock On, Won't Operation On.
Check For Open Circuit Ip902 In Power Supply. P. No. 95kpjc0284zz. Check For Short Circuit Or Faulty C1589, 1000µf 16v, On Tuner Pcb.
SHARP
VC585
E-e Picture Distorted.
C211 (10 Uf/16v) Inside If Module.
SHARP
VC585
Ee Picture Distorted
C211 10µf/16v In If Module
SHARP
VC585
Hum And Pattern Interference In Ee And Play. High Freq. Oscillations On +12 & +9v Rails
Replace C913,917,918,919 And C916 In Power Supply.
SHARP
VC6300
Sound Wowing.
Check Capstan Motor Speed By Selecting Record And Adjust R794 For Zero Volts On Tp713, If Tp721 Exceed 500 Millivolt P-p Ripple, Change Motor.
SHARP
VC6300
Turns Off While Recording Or Switches Off After 6 Inches.
Check For Take-up Reel Rotation, Or The Machine Thinks So. Check That The Reel Isn't Stopping - If It Does Clean Belts And Tyres And Replace The Clutch. If The Reel Isn't Stopping Check The Output From The Sensor Af4: It Should Be 5-10v P-p, If Not Repla
SHARP
VC651
Capstan Goes To Half Speed
Clean Ctrl Track Head With Pcb Cleaner. Low Control Track Forces Capstan Servo To Half Speed Mode.
SHARP
VC651
Capstan Runs Fast In Record
Diode In Syscon Faulty(leaky) D814
SHARP
VC651
Capstan Too Fast
Check Fg Pulse Dj's Plug A1
SHARP
VC651
Capstan Too Fast.
Check Fg Pulse, Dj's Around Plug A1.
SHARP
VC651
Chews Tapes, Intermittent No Take Up Torque.
Reel Brake Not Releasing, Mode Switch Faulty.
SHARP
VC651
Chews Tapes, Poor T/u Torque.
Reel Brake Not Releasing. Mode Switch?
SHARP
VC651
Int Capstan Lock
Cracks Around Screws Holding Pcb-a
SHARP
VC651
Int Capstan Lock.
Craks Around Screws Holding Pcb-a.
SHARP
VC651
See Vc685
SHARP
VC651
Slow Capstan Speed
Pinch Roller In Engaging. Lubricate Pivot.
SHARP
VC681
Cassette Loads Up & Down At Power On By Itself ?
R822 Dj's Or O/c On Mother Pcb
SHARP
VC681
Cassette Loads Up And Down At Power On By Itself.
R822 Dj's Or O/c On Mother Pcb.
SHARP
VC681
Chews Tapes
Loading Belt
SHARP
VC681
Chews Tapes.
Loading Belt Faulty.
SHARP
VC681
Loads Or Eject But No Functions
End Sensor O/c
SHARP
VC681
No Chroma In Record
Chroma Delay Line.
SHARP
VC681
No Chroma On Record.
Chroma Delay Line.
SHARP
VC681
Records Ok ,ee Ok But Mutes Video And Audio
No Pb 5v. C413 On Luminance/chroma Sub Board S/cct.
SHARP
VC681
See Vc685
SHARP
VC681
Will Load And Eject But No Other Functions.
End Sensor O/c.
SHARP
VC681
Wont Load Or Eject. Interm Doing Either.
Reposition The Mode Control Switch.
SHARP
VC682
Capstan And Reel Go Forward In Rewind Mode
Plug A1 Pin 8 Dj'd
SHARP
VC682
Capstan And Reels Go Forward In Rewind.
Plug A1 Pin 8 Dj'd.
SHARP
VC682
Capstan Slows Down
Isolate Pin 13 Of Ic703 And Connect To Earth.
SHARP
VC682
Capstan Slows Down.
Isolate Pin 13 Of Ic703 And Connect To Earth.
SHARP
VC682
No Functions
R916 O27 In Psu
SHARP
VC682
No Functions.
R916 (.27 Ohm) In Psu.
SHARP
VC682
No Load Motor
Ic802 Ta7288
SHARP
VC682
No Load Motor Drive.
Ic802 (ta7288).
SHARP
VC682
No Play Functions
Ic801
SHARP
VC682
No Play Functions.
Ic801 (rh-ix0151gezz).
SHARP
VC682
Won't Load/eject.
R907 (.27 Ohm) In Psu O/c.
SHARP
VC682
Wont Load/eject
R907 O27 In Psu
SHARP
VC682X
When In Rec. Pause Mode, Wont Rec.
Replace Mode Select Switch.
SHARP
VC685
Brakes Don't Lock Hubs On Eject,
Pin From Underneath Slider Panel Has Fallen Out.
SHARP
VC685
Looks Like Worn Idler
Brake Solenoid Underneath Plugs Into Reel Sensor Pcb Not Working
SHARP
VC685
No Clock Display
Ic5001 Pwb-i
SHARP
VC685
No Clock Display.
Ic5001. (rh-ix0164gezz) On Pwb-1.
SHARP
VC685
No Picture In Playback
Missing Pb 5v Q808 Replace C413 (100µf/10v) On Y/c Module Board (rhs).
SHARP
VC685
Reel And Capstan Run Backward
Clock Xtal For Ic801 R/s
SHARP
VC685
Reel And Capstan Run Backwards, Vcr Won't Turn Off.
Clock Xtal For Ic801 Faulty.
SHARP
VC685
Similar Symptoms To Worn Reel Idler.
Brake Solenoid Underneath Plugs Into Reel Sensor Pcb Not Working.
SHARP
VC685
Vcr Wont Turn Off
Clock Xtal Faulty For Ic801
SHARP
VC685X
Wont Eject Tapes Chews Tapes.
Replaced Filter Fl801.
SHARP
VC7300
Capstan Motor Will Not Operate.
Replaced Q809.
SHARP
VC7300
Capstan Won't Operate.
Q809 (2sd687).
SHARP
VC7300
Capstan Wont Operate.
Q809 (2sd687).
SHARP
VC7300
Capstan Wont Work
Q809 2sd687
SHARP
VC7300
Cassette Loading Motor On At All Times.
Check Q8811 2sd687
SHARP
VC7300
Cassette Motor On All Time
Q809 2sd687
SHARP
VC7300
Cassette Motor On At All Time.
Q809 (2sd687).
SHARP
VC7300
Cassette Motor On At All Time.
Q809 (2sd687)
SHARP
VC7300
Chopper Tranformer Squealing
Change C920 (10mfd 50v)
SHARP
VC7300
Dew Sensor On
Q805 Q806 2sc1815
SHARP
VC7300
Dew Sensor On All The Time.
Q805, Q806 (2sc1815).
SHARP
VC7300
Dew Sensor Operating With No Moisture Present.
Replace Q805 And Q806.
SHARP
VC7300
Dew Sensor Problems.
Check Q805 And Q806, 2sc1815.
SHARP
VC7300
Drum Rotates At All Times, No Functions.
Check Loading Ring Position And Reset If Necessary.
SHARP
VC7300
Drum Rotates At All Times, No Inject Or Eject.
Check Mechanical Loading Ring Position.
SHARP
VC7300
Drum Rotates No Functions
Check Loading Ring Position & Reset If Necc
SHARP
VC7300
Functions Ok But No Eject
Lever #23 Rhs Eject Mech Lubricate
SHARP
VC7300
Functions Ok But Won't Eject Tape.
Lever (no 33 On Parts List) On Rhs Of Front Loader Sticking, Lubricate.
SHARP
VC7300
Ghosting Picture Appears After A Few Hrs. Operation On E-e
Freeze Sf1501 Filter On Tuner I.F. Board If Picture Comes Good Replace Filter.
SHARP
VC7300
Int B/w Picture On Playback. Audio Ok.
Check If Main Solenoid Releases When Stop Is Pressed. If Not Solenoid Could Need Lubrication.
SHARP
VC7300
Int Pulsing Of Aux. Motors.
Change Regulator Trans 2sc1212a To A Bd139 With Moderate Heat Sink.
SHARP
VC7300
Int Recording.
Check Ic1301 Pin 8 For Int Loss Opf Signals.
SHARP
VC7300
Loading Motor Weak.
Change Q8091.
SHARP
VC7300
Loading Motor Won't Rotate.
Look For Thermal Output To Main Solenoid O/c.
SHARP
VC7300
Loss Of Colour On Pre-rec. Playback Of Own Rec. Ok.
Fit 270 Pf In Parallel With C540. Fit 1.8k Ohms 1/4w In Parallel With R522.
SHARP
VC7300
No 12 V Rail
R903 O27 Fuse
SHARP
VC7300
No 12 Volts At Tp901.
Replaced R903.
SHARP
VC7300
No 12v At T.P. 901.
On Vc7300 Check R903 0.27 Ohms. On Vc7700 Check R912 0.27 Ohms Q904 2sd1128.
SHARP
VC7300
No 12v From Power Supply.
Check R903 (.27 Ohm Fusible).
SHARP
VC7300
No Capstan Motor Drive.
Check Q809, 2sd687.
SHARP
VC7300
No Func.Only Eject/load, Head Drum Running Continuously.
Check Faulty Unload Or After load Switch. Sw01 And Sw02 On The Deck.
SHARP
VC7300
No Power Indication, No Clock Fuse F902 O/c.
Change Q908 With 2sc1826 Q920 10 Mfd 50v Q942 10 Mfd 16v
SHARP
VC7300
No Power No Clock
Q908 2sc1212 C916 10µf
SHARP
VC7300
No Power, No Clock.
Q908 (2sc1212) Also Replace C916 (10 Uf).
SHARP
VC7300
No Power. Clock Inoperative.
Replaced Q908, C920 And C942.
SHARP
VC7300
No Servo Lock In Play
X502 Rcrsa0011 Or Ic504 An6342
SHARP
VC7300
No Servo Lock On Play.
X502 (rcrsa0011) Or I504 (an6342n).
SHARP
VC7300
Picture Rolling On E-e And Record.
Check I.F. Package Cct's Output If Ok Check C438 (47 Mfd) Gone Low.
SHARP
VC7300
Poor Or No Colour When Tapes Rec. On Other Mach. Own Rec Ok
Fit A 270pfd In Parallel With C540 And Fit 1.8 Kohm In Parallel With R522 Then Check Chroma Oscillator Frequency.
SHARP
VC7300
Suddenly Turns Off.Play/rec. Restores Normal Functions.
Check Take-up Spool Is Stopping. If It Is, Check The Play Idler May Need Replacement. If The Spool Doesn't Stop, The Cassette Lamp Could Just Be Responsible (intermittently O/c) Or Take-up Rotation Sensor Opocoupler Assembly Is Faulty.
SHARP
VC7300
Tangles Or Chews Tapes When Ejected. Prevalent After Rew.
Replaced Load Belt.
SHARP
VC7300
Tape Looping After Rewind.
Replace T/u Turntable, Main Brake And Idlers And Check Main Brake Torque As Per Service Manual.
SHARP
VC7300
Tape Wont Load. Head Drum Rotates When Play Is Selected.
Put Loading Ring Assy In Correct Position And Sequence.
SHARP
VC7300
Won't Accept Or Inject Cassette.
Check Q8811 Or D313.
SHARP
VC7300
Won't Accept Tape.
Switch On Front Loading Mechanism Pt No: Qswt0001gezz.
SHARP
VC7300
Wont Accept Tapes
Switch On Front Loading Mech P# Qswt0001gezz
SHARP
VC7700
Cassette Loading Motor On At All Times.
Check Q8811 2sd687
SHARP
VC7700
Chopper Tranformer Squealing
Change C920 (10mfd 50v)
SHARP
VC7700
Dew Sensor Problems.
Check Q805 And Q806, 2sc1815.
SHARP
VC7700
Drum Rotates At All Times, No Inject Or Eject.
Check Mechanical Loading Ring Position.
SHARP
VC7700
Int Ejects Tapes, Flap Opening Int. Without A Tape In.
555 Timer Ics On Mechanon Board Faulty.
SHARP
VC7700
Int Recording.
Check Ic1301 Pin 8 For Int Loss Opf Signals.
SHARP
VC7700
Laces Up Then Unlaces.
Change Slack Sensor On Pinch Roller Bracket.
SHARP
VC7700
Loading Motor Weak.
Change Q8091.
SHARP
VC7700
Loading Motor Won't Rotate.
Look For Thermal Output To Main Solenoid O/c.
SHARP
VC7700
Loss Of Colour On Pre-rec. Playback Of Own Rec. Ok.
Fit 270 Pf In Parrallel With C540. Fit 1.8k Ohms 1/4w In Parallel With R522.
SHARP
VC7700
No 12v At T.P. 901.
On Vc7300 Check R903 0.27 Ohms. On Vc7700 Check R912 0.27 Ohms Q904 2sd1128.
SHARP
VC7700
No Capstan Motor Drive.
Check Q809, 2sd687.
SHARP
VC7700
No Play F.F. Rew. Or Rec.
Replaced Capstan Motor.
SHARP
VC7700
No Power Indication, No Clock Fuse F902 O/c.
Change Q908 With 2sc1826 Q920 10 Mfd 50v Q942 10 Mfd 16v
SHARP
VC7700
Refer Vc7300
SHARP
VC7700
See Vc7300
SHARP
VC7700
Tangles Or Chews When Ejected. Prevalent After Rew.
Replaced Load Belt.
SHARP
VC7700
Won't Accept Or Inject Cassette.
Check Q8811 Or D313.
SHARP
VC7700
Won't Turn Off. Cass. Lamp On,head Drum Rotates.
Check Failure Of Unload End Switch Sw 1. If The Tape Guides Have Not Retracted Fully, Check The Loading Mechanics Starting With The Loading Motor Belt.
SHARP
VC7750
Cassette Loading Motor On At All Times.
Check Q8811 2sd687
SHARP
VC7750
Chopper Transformer Squealing
Change C920 (10mfd 50v)
SHARP
VC7750
Dew Sensor Problems.
Check Q805 And Q806, 2sc1815.
SHARP
VC7750
Drum Rotates At All Times, No Inject Or Eject.
Check Mechanical Loading Ring Position.
SHARP
VC7750
Int Recording.
Check Ic1301 Pin 8 For Int Loss Opf Signals.
SHARP
VC7750
Loading Motor Weak.
Change Q8091.
SHARP
VC7750
Loading Motor Won't Rotate.
Look For Thermal Output To Main Solenoid O/c.
SHARP
VC7750
Loss Of Colour On Pre-rec. Playback Of Own Rec. Ok.
Fit 270 Pf In Parrallel With C540. Fit 1.8k Ohms 1/4w In Parallel With R522.
SHARP
VC7750
No 12v At T.P. 901.
On Vc7300 Check R903 0.27 Ohms. On Vc7700 Check R912 0.27 Ohms Q904 2sd1128.
SHARP
VC7750
No Capstan Motor Drive.
Check Q809, 2sd687.
SHARP
VC7750
No Power Indication, No Clock Fuse F902 O/c.
Change Q908 With 2sc1826 Q920 10 Mfd 50v Q942 10 Mfd 16v
SHARP
VC7750
Refer Vc7300
SHARP
VC7750
See Vc7300
SHARP
VC7750
Won't Accept Or Inject Cassette.
Check Q8811 Or D313.
SHARP
VC781
Int Stops In Rew/ff.
Earth Cassette Slider By Fitting Spring (mspro113gefj)
SHARP
VC782
Fails Recording After Pause.
Replace Load Belt.
SHARP
VC782
Hum On Ee Audio.
Ic601 In Audio Board
SHARP
VC782
Supply Guide Comes Back And Gets Caught On Back Tension Arm.
Replace Loading Gear Under Supply Guide
SHARP
VC787
Operate Light Goes Out After 8 Seconds
Check F902 Ur15v Rail
SHARP
VC8300
Agc On Monitor Only Ok In Playback.
Q1507 No Base Voltage Due To R1540 Being O/c Or High.
SHARP
VC8300
Agc Or Negative Picture.
Fl4401 S/c.
SHARP
VC8300
Blowing Fuse F803. Wont Accept Or Eject Tape.
Replace Eject Motor.
SHARP
VC8300
Cap. Speed Varying. Wow In Sound. Servo Phase Signal Faulty
Remove Bridge 1704 On P.W.B.-a. Change It With 680k Ohms And O.O22 Mfd In Parallel.
SHARP
VC8300
Capstan Running Fast.
Q718, Q719 S/c.
SHARP
VC8300
Capstan Slows When Hot Noise Band In Pb
C729 10µf
SHARP
VC8300
Capstan Slows When Hot, Noise Band Thru Picture.
C729 (1ouf Tan).
SHARP
VC8300
Capstan Speed Varies, Wow In Sound.
Check Bridge I704 On Pwb A.
SHARP
VC8300
Capstan Varies Speed Wow In Audio
Check Bridge I704 On Pwb-a
SHARP
VC8300
Cassette Loads But Not Threading.
Q714, Q716, Q717 S/c.
SHARP
VC8300
Cassette Will Not Load Or Unload Or Eject.
1. Check For 25v Present On Loading Motor. 2. Check For Faulty Ry801 Load/unload Switch.
SHARP
VC8300
Cassette Will Not Load.
Cassette Down Switch S2 Broken.
SHARP
VC8300
Chews Or Tangles Tape When Ejected.
Replace Rubber Boot On Take Up Brake Arm.
SHARP
VC8300
Drum Fails To Start.
Drum Motor Int. Rmotp101pgezz.
SHARP
VC8300
Drum Wont Start
Drum Motor Int P# Rmotp1019gezz
SHARP
VC8300
Ejects After Loading Up.
Change Loading Belt.
SHARP
VC8300
Horizontal Noise Bars.
1. Capstan Running Slow - Ic1703 2. Dry Joint Thick-film Cr503. 3. Reset D Lock (r711)
SHARP
VC8300
Int Blows F903 When Unlacing.
Faulty Drum Motor Or Forward/reversee Switch Int. Shorting. (p.No. Qsw-10002ge).
SHARP
VC8300
Int Colour Or Lum In Record
Ic301 Sa8063
SHARP
VC8300
Int Loss Of Playback Picture (blank Screen)
Look For D/j's On Plug/socket Converter Cd On Pwb-c.
SHARP
VC8300
Int Stops In Play After Lace Up
Main Solenoid Sticking. Lub Or Replace
SHARP
VC8300
Int Stops In Play/record
Slack Sensor Faulty
SHARP
VC8300
Int Stops On Play After Lace-up.
Main Solenoid Sticking - Lubricate Or Replace.
SHARP
VC8300
Inter. Blows Fuse F903. Blows When Tape Unthreading.
Check Faulty Drum Motor. Check Intermittent Short In The Forward/reverse Switch (part No. Qswf0002ge). Mounted Near The Solenoids.
SHARP
VC8300
Interm. Colour Flashing Of Self Rec.
Replaced Ic301.
SHARP
VC8300
Intermittent Colour Flashing On Playback Of Own Recording.
Change Ic301 Rec. Amp. Vhisa 8063//-1.
SHARP
VC8300
Intermittently Drum Fails To Start In P/back Or Record.
Change Int. Drum Rmotp1019gezz.
SHARP
VC8300
Intermittently Stops In Play And Record.
Slack Sensor Faulty.
SHARP
VC8300
Intermittently Stops On P/back Or Rec. After Lace Up.
Change Main Solenoid Plunger Rplu0046gezz.
SHARP
VC8300
Lines Across Pict. And Sound Wavering.
Capstan Motor Faulty.
SHARP
VC8300
Loads Up And Ejects Tape.
Check For Craks In Connector Panel Below Solenoids (at Front Of Deck).
SHARP
VC8300
Machine Stops In Laced Up Position.
Solenoid Sticking Need Lubricating.
SHARP
VC8300
No "fast Forward"
Spring (49) Fallen Off.
SHARP
VC8300
No Audio In Ee
I1502 Ix0043
SHARP
VC8300
No Capstan Drive
Q718,q719,q720,q721,q723
SHARP
VC8300
No Capstan Drive.
Q721 (2sd880) In Capstan Brake.
SHARP
VC8300
No Capstan Lock
Tracking Pot Or Track To Pot O/c
SHARP
VC8300
No Capstan Lock.
Tracking Pot Or Pc Board To Pot Open Circuit.
SHARP
VC8300
No Capstan Motor Drive.
Replace All Q718, Q719, Q720, Q721, Q723.
SHARP
VC8300
No Capstan Motor Drive.
Check Q718. If Faulty Also Check Q719, Q720 Q723 And D711. Transistor Substitutes: Q714, 715 And Q 718, 719 Were 2sc2021. Use 2sc945aq. Q716 And Q720, 723 Were 2sa933. Use 2sa733 Or 2sa950y.
SHARP
VC8300
No Colour.
1. Ic1505. 2. Cr501. 3. Check Pin 3 Of Pugcb, Adjust Chroma Current Control On Head Amp.
SHARP
VC8300
No Drum Motor Drive
Replaced Q714,q715,q716,q717
SHARP
VC8300
No Drum Motor Drive.
Replace Q714, Q715, Q716, Q717.
SHARP
VC8300
No Drum Motor Drive.
Check Q714. If Faulty Also Check Q715 And Q716. transistor Substitutes: Q714, 715 And Q718, 719 Were 2sc2021. Use 2sc945aq. Q716 And Q720, 723 Were 2sa933. Use 2sa733 Or 2sa950y.
SHARP
VC8300
No Pic On Record/play.
L405 Faulty Or Ic1402 (ha11703).
SHARP
VC8300
No Picture In Play/record
L405 Or Ic1402 Ha11703
SHARP
VC8300
No Picture In Playback.
Change C439 If Fault Still Present Change Ic402.
SHARP
VC8300
No Sound On E-e
I1502 (ix0043).
SHARP
VC8300
No Sound On Own Recordings Pre-recorded Tapes Ok.
Ic601 Faulty.
SHARP
VC8300
Noisy Picture After Playing A Pre-recorded Tape Sev. Times.
Check Erase Osc If Partly Operating On Playback, If So Ic601 Faulty.
SHARP
VC8300
On Playback Looks Like A Capstan And A Drum Servo Fault.
Check C731 10 Mfd Tant For Leakage Ic702, Ic703 Etc.
SHARP
VC8300
Overshoot On Black To White Transitions On Own Recordings.
Check Deviation Level Adjustment.
SHARP
VC8300
Patterning On Ch4 Or Snowy On Ch3 Output Of Rf Converter.
Faulty Rf Converter.
SHARP
VC8300
Ripple In Sound.
1. Faulty Capstan Motor. 2. Worn/corrugated Pinch Roller.
SHARP
VC8300
Smeary Picture.
C4413 Or Video-board Dry Joint.
SHARP
VC8300
Snowy Pic On Tuner And Play.
Q1201 (2sc2570) In Rf Booster.
SHARP
VC8300
Snowy Picture In All Modes
Q1201 2sc2570 In Rf Booster
SHARP
VC8300
Snowy Picture On Tuner And/or Playback.
Q1201 In Rf Booster Unit. Use Toshiba 2sc2753.
SHARP
VC8300
Snowy Picture.
Q1201 In Modulator S/c.
SHARP
VC8300
Stops Int
Reel Motor Or/and Q6006 2sd687
SHARP
VC8300
Stops Intermittently.
Check Reel Motor And Q6006 (2sd687).
SHARP
VC8300
Tangles Tape On Eject.
Change Brake Rubber On Take-up Side Reel. Pgumm0012gezz.
SHARP
VC8300
Tape Stops In Play
Pinch Solenoid Not Operating. Check Fuse Under Inslulation On Solenoid
SHARP
VC8300
Tape Stops In Play Mode.
Pinch Solenoid Not Operating, Check Fuse Under Insulation On Solenoid.
SHARP
VC8300
Tapes Getting Chewed.
Worn Out Brushes In Reel Motor - Change Reel Motor. intermediate Drive Wheel For Supply And Take Up Spools Seized. Rough Edges On Guide Slots For Intermediate Drive Wheel - Smooth Off Roughness Very Carefully Without Enlarging Slots. This Fault Usually
SHARP
VC8300
Tapes Tangle On Eject
Replace Brke Rubber On T/u Reel
SHARP
VC8300
Tapes Tangle On Eject.
Replace Brake Rubber On T/u Reel.
SHARP
VC8300
To Operate Mechanism With Top Servo Pcb Up.
Remove Plug Ao On Servo Pcb.
SHARP
VC8300
Tracking Drifting Over A Couple Of Weeks.
Change Capstan Motor.
SHARP
VC8300
Will Not Eject From Carriage,wont Allow Carr.To Drop Correc
Check Lock Off Lever (for Releasing Cassette Flap Broken), Or Has Been Forced Out Of Position. Change Lock Off Lever.
SHARP
VC8300
Will Not Rewind
Gear Fallen Off Vs Reel-motor.
SHARP
VC8300
Won't Load Or Unload.
Change Loading Motor Ic1805 Sta401 Motor Changeover Switch (p.No. Qsw-10002ge).
SHARP
VC8300
Won't Play "c" Size Cassette Adaptor.
Adjust Slack Sensor (vr844) On On Pwb-a.
SHARP
VC8300
Won't Switch Off.
Check Q902 S/c.
SHARP
VC8300
Wont Play Vhsc Tape In Adaptor
Adjust Slack Sensor Vr844 On Pwb-a
SHARP
VC8300
Wont Tune To Stations.
Check Aux/tuner Switch Faulty.
SHARP
VC8300
Wow And Flutter. No Capstan Servo.
Check Bridge On Pwb A And Or Replace With Original Part.
SHARP
VC8300
Wow In Audio
Capstan Belt Or Dry Bearings
SHARP
VC8300
Wow In Sound.
Capstan Belt, Or Dry Bearings In Motor.
SHARP
VC8300
Z Paid
SHARP
VC8452
No Or Intermittent Reel Drive In All Modes.
Change Ic705, (ta7267p)
SHARP
VC8482
No High Band On Tuner.
R958 (2.7k0 In Psu.
SHARP
VC8482
No High Band Tunner
R958 2.7k In Psu
SHARP
VC8482
No Picture In Cue/rewind
Ic704 Td62104
SHARP
VC8482
No/int Reel Drive
Ic705 Ta7647
SHARP
VC8482
Won't Accept Cassette.
Check Operation Of Cass. Down Switch. Pin 1 Of Plug Aa, Cass. Down (l) Should Be (h) With No Cassette In.
SHARP
VC8482
Won't Accept Cassette. Operation Faulty.
If The Main Cam Gear On The Underside Of Mechanisim Is Wound Fully Clockwise Then Rotate, By Use Of The Loading Motor Worm, 180 Deg Counter Clockwise. A. If Then All Operations Perform Without Faulty Replace Suspect C818, 10µf 16v, On
SHARP
VC8581
Intermittent Recording.
Check Ic401 (ha11744nt1) Video Processor For Luminance At Pin 20 And Fm Out. Osc Signal At Pin 12 To Video Heads.
SHARP
VC9100
Interm. Chewing, Cuts Off On P/back And Record.
Check If Reel Idler Ok, Replace Int. Reel Motor. Rmotv1008gezz.
SHARP
VC9100
Interm. White Lines Break Up Of Pic. On E-e And P/back.
Only On Rf Out Not Video Out. Replace Ic403 On Y/c Pcb.
SHARP
VC9100
Loses Colour On Recordings
Change Filter Fl504 Rmptdoo52gezz.
SHARP
VC9100
No Picture In Ee Or Playback.
Replaced Ic403 On Video Pcb.
SHARP
VC9100
No Power, No Clock.
No 240v To Mains Transformer? Check R901, Change C901 (.1 Mfd). If Voltage To Power Supply Change C9009 (10 Mfd 63v).
SHARP
VC9100
No Reel Motor Voltage.
Change Q8001 (2sd880).
SHARP
VC9100
No Reel Torque On Playback Or Record.
Change Q7754 2sd882 And Add 27 Ohm Collector To Emitter.
SHARP
VC9100
No Reg. 12v Pin 2 Ae.
Check R9019 (15 Ohms). Check Q9006 Use (2sc1826).
SHARP
VC9100
No Video On E-e Mode.
Change C204 (220mfd 10v).
SHARP
VC9100
Picture Un Stable On Some Channels.
Replace Zener Ic, 11401, Rhix0037gezz.
SHARP
VC9100
Poor Or No Luminance
Change Ic403
SHARP
VC9100
Refer Vc9300
SHARP
VC9100
Rf Interf. On Low Ch. Under Weak Signal Conditions.
Remove R9004 And C9006.
SHARP
VC9100
See Vc9300
SHARP
VC9300
Blows 2.5 A Sb Fuse On Rear Of Vcr
Q9002 In Psu Or Reel Motor If '02' Type
SHARP
VC9300
Blows 2.5a Sb Fuse At Rear Of Vcr.
Q9002 In Psu.
SHARP
VC9300
Blows Fuse On P/supply 12v Rail Goes 25v.
Replace R16 In P/supply And Remove Glue From Pcb.
SHARP
VC9300
Cass. Will Not Eject, Won't Allow Carriage To Drop Corre.
Check Lock Off Lever (for Releasing Cassette Flap Broken), Or Has Been Forced Out Of Position. Change Lock Off Lever.
SHARP
VC9300
Cassette Will Not Eject.
Door Flap Not Opening Fully Due To Bent Lever Angle Assembly.
SHARP
VC9300
Chewing Tapes.
Cassette Down-end (csd) Switch Broken, Or Reel Motor.
SHARP
VC9300
Chews Tapes Int , Stops In Play
Reel Motor Rmotv1008gezz
SHARP
VC9300
Clock Display Shows Two Days
Ic5001
SHARP
VC9300
Distorted Or No Pic On E-e.
Q721 (2sb4568) On Pwb-a.
SHARP
VC9300
Distorted Picture In Ee
Q721 2sd468 Pwb-a
SHARP
VC9300
Drum Moor On All The Time.
Remove Glue On Q717 And Q718.
SHARP
VC9300
Drum Speed Int
X502
SHARP
VC9300
Drum Spins All Time
Remove Glue On Q717, Q718 Or Q718 Faulty.
SHARP
VC9300
Drum Turns All The Time.
Q717 (2sc945)
SHARP
VC9300
For Low Reel Torque In All Modes.
Check For D/j's On Q8001, Located At Rear Of Chassis, By The Head Drum.
SHARP
VC9300
Goes To Stop As Soon As It Is Fully Loaded.
Ic2002 On Pwc "d". Head Switching Pulses Low In Amplitude.
SHARP
VC9300
Grey Washed Out Pic In Play
Ic401
SHARP
VC9300
Int Blows 2.5a Fuse At Rear Of Vcr.
Change Reel Motor If "02" Type.
SHARP
VC9300
Int Capstan Speed
Ic703
SHARP
VC9300
Int Capstan Speed After 1-2 Hours
Ic703
SHARP
VC9300
Int Chews Tapes Or Cuts Out In Play/record.
Reel Motor Int (rmotv1008gezz).
SHARP
VC9300
Int Colour
Ic503
SHARP
VC9300
Int Colour And Drum Speed
Ic504
SHARP
VC9300
Int Colour On Recordings.
Fl504 (doo52ge).
SHARP
VC9300
Int Erratic Behaviour
Ic801 Cpu
SHARP
VC9300
Int No Power/ Stops
Q808
SHARP
VC9300
Int Play Or Record.
Change Idler Assembly And Check For Lazy Drum Motor.
SHARP
VC9300
Int Play Pic
Fl401
SHARP
VC9300
Int Reel Motor Slows
R7733
SHARP
VC9300
Int Stops
C719 Leaky
SHARP
VC9300
Interm. Chewing, Cuts Off On P/back And Record.
Check If Reel Idler Ok, Replace Int. Reel Motor. Rmotv1008gezz.
SHARP
VC9300
Interm. White Lines Break Up Of Pic. On E-e And P/back.
Only On Rf Out Not Video Out. Replace Ic403 On Y/c Pcb.
SHARP
VC9300
Intermittent Colour On Playback.
1. D/j On C534. 2. Cracked P.C. Board Near Centre Retaining Screw Around R538.
SHARP
VC9300
Intermittent No Power.
D/j Mains I/p Board.
SHARP
VC9300
Intermittent Wow On Sound.
Change R745. Check Also For D/j's Around Ic7753 And C788 (leaky).
SHARP
VC9300
Intermittently Shuts Down. No Functions No Display
C903 Low Capacitance. (47uf 16v Servo/sys Con Pcb)
SHARP
VC9300
Loses Colour On Recordings
Change Filter Fl504 Rmptdoo52gezz.
SHARP
VC9300
Low Reel Motor Torque
Q7754 2sd882
SHARP
VC9300
Low Reel Motor Torque On Play And Record.
Q7754 (2sd882).
SHARP
VC9300
Low Reel Torque In All Modes.
Look For D/j's On Q8001 Located At Rear Of Chassis Along Side Head Drum.
SHARP
VC9300
Mains Fuse Blown (f9001 2.5a)
Check Q7754 For O/c And R7758 (27 Ohm), Change Q903 And D901 On Mechanon Board.
SHARP
VC9300
No "stop" Function.
Poor Connection Plug Ha.
SHARP
VC9300
No 12v Reg From Psu
R9019 15O , Q9006 2sc1983
SHARP
VC9300
No Capstan Drive
Plug Ad Crimped
SHARP
VC9300
No Colour Int In Record
Fl504 D0052ge
SHARP
VC9300
No E.E. Picture.
Check Q721 O/c In Tuner, Use Bc337.
SHARP
VC9300
No Eject
Ic801
SHARP
VC9300
No Output From Modulator.
Check L2 O/c (12 Volt Supply).
SHARP
VC9300
No Picture - No Sound.
Tuner/aux. Switch In Aux./position.
SHARP
VC9300
No Picture In Ee Mode.
Replaced C204 (220 Mfd 10v).
SHARP
VC9300
No Picture In Ee Or Pb
Fl202
SHARP
VC9300
No Picture In Ee Or Playback.
Replaced Ic403 On Video Pcb.
SHARP
VC9300
No Picture In Playback.
Change C439 If Fault Still Present Change Ic402.
SHARP
VC9300
No Power
F9001 O/c Q9001 Shorted
SHARP
VC9300
No Power, No Clock.
No 240v To Mains Transformer? Check R901, Change C901 (.1 Mfd). If Voltage To Power Supply Change C9009 (10 Mfd 63v).
SHARP
VC9300
No Reel Drive
Q8001 2sd880
SHARP
VC9300
No Reel Drive In Pb/rec But Ff/fr Ok
Q7754
SHARP
VC9300
No Reel Motor Drive.
Q8001 (2sd880).
SHARP
VC9300
No Reel Torque On Playback Or Record.
Change Q7754 2sd882 And Add 27 Ohm Collector To Emitter.
SHARP
VC9300
No Reg 12v From Power Supply.
R9019 (15 Ohm) Q9006 (2sc1983).
SHARP
VC9300
No Reg. 12v Pin 2 Ae.
Check R9019 (15 Ohms). Check Q9006 Use (2sc1826).
SHARP
VC9300
No Reverse Search With Tape Inserted.
Change Reel Motor.
SHARP
VC9300
No Rew., F.F Ok. Pressing Rewind Again Produces F.F. & Rew.
Check R7751 Relay Sticking.
SHARP
VC9300
No Rewind
Ry7751
SHARP
VC9300
No Sound. In E.E. And Playback.
Faulty Rf Converter - Replace.
SHARP
VC9300
No Video On E-e Mode.
Change C204 (220mfd 10v).
SHARP
VC9300
Noise Bars Floating Through Picture - No Colour On Play.
X502 (4.43 Mhz) Xtal Faulty. Divided Down For 50 Hz Reference In Capstan Servo, Phase Lock Etc. Can Also Be Failure Of Ic504 (an6342n).
SHARP
VC9300
Noise Bars Move Slowly Through The Pic. Sound Doesn't Wow.
Check The Capstan Lock Voltage At Tp3 When The Flywheel Is Slowed By Hand, It Doesn't Alter. Usually Waveform Tp1 Is Missing, Due Either To D707 Being Leaky Or R475 (82 K Ohm) O/c. If The Drum And Capstan Servos Are Both Wowing, Check That The Pb 50hz Si
SHARP
VC9300
Noise On Cue
Lub Roller Asy #17 In Parts List
SHARP
VC9300
Noisy Picture On Own Recording.
Mono Multi Q702/q703 Out Of Adjustment. Adjust R709.
SHARP
VC9300
Not Erasing On Record
C611 C512
SHARP
VC9300
On Rec. Noise Bars Floating Through Pic.
Not Recording Control Pulses On Tape When Recording C717 (.33 Mfd Tant) Faulty. Also Can Be Failure Of I.C. 701 (an6344).
SHARP
VC9300
Pic And Audio Muted On Pause
Q817
SHARP
VC9300
Pic Unstable In Ee
Zener I1401 Ix0037ge
SHARP
VC9300
Pic Unstable On E-e
Zener Ic I1401 (ix0037ge).
SHARP
VC9300
Picture Un Stable On Some Channels.
Replace Zener Ic, 11401, Rhix0037gezz.
SHARP
VC9300
Plays For Three Sec. Then Motors Stop.
Int After Load Switch.
SHARP
VC9300
Poor Or No Drum Rotation
Ic704 M51724p Drum Current Driver
SHARP
VC9300
Poor Or No Luminance
Change Ic403
SHARP
VC9300
Poor Picture In Ee & Play
Ic403 Iz0008ge
SHARP
VC9300
Poor Picture No Luminance.
Replaced Ic403.
SHARP
VC9300
Poor Picture On E-e And Play.
Ic403 (iz0008ge).
SHARP
VC9300
Poor Recorded Picture.
C204 (22ouf)
SHARP
VC9300
Recorded Picture Poor
C204 220 µf
SHARP
VC9300
Rf Interf. On Low Ch. Under Weak Signal Conditions.
Remove R9004 And C9006.
SHARP
VC9300
Stops After 30 Minutes On Playback
If Fault Occurs In Play Or Record But Not Fast Wind,check Drum Pick Up Head.
SHARP
VC9300
Stops As Soon As Laced Up
Ic2002 Pcw-d Head Sw Pulse Low
SHARP
VC9300
Stops For No Reason And /or Chewing Tapes.
Capstan Bearing Is Binding. Remove, Clean And Lubricate Capstan Flywheel Bearing.
SHARP
VC9300
Tape Jammed.
Cassette Cover Release Spring (4) Fig. 35 Is Bent - Replace.
SHARP
VC9300
Tape Speed Varies.
S/h O/p (9) Ic703 Permanently Around 10v. Replace Ic703.
SHARP
VC9300
Tape Spills Out From The Supply Reel: Wont Rew. At End.
Check Reel Motor Faulty And Will Not Work Under Full Load, Or Reel Idler Wheel Binding On Shaft Or Chassis And/or Clutch Binding, Faulty Slide Switch.
SHARP
VC9300
Tapes Getting Chewed.
Worn Out Brushes In Reel Motor - Change Reel Motor. intermediate Drive Wheel For Supply And Take Up Spools Seized. Rough Edges On Guide Slots For Intermediate Drive Wheel - Smooth Off Roughness Very Carefully Without Enlarging Slots. This Fault Usually
SHARP
VC9300
The Cassette Housing Stops Half Way.
Check Eject Finish Switch On The Cassette Housing For O/c.
SHARP
VC9300
Unit Dead.
1. Fuse F901 Loose - Adjust Holder For Firm Grip Of Fuse. 2. Q9003, Q9002 S/c.
SHARP
VC9300
Very Poor Playback Picture.
No Signal From One Head, Look For D/j On Rotating Transformer.
SHARP
VC9300
White Out On Ee
R239 Dj'd
SHARP
VC9300
Won't Play, Rew Or F.F. Record Ok.
Check Output At Ad4, If So D/j Under Plug Ha13 Or Crack In Cct Board.
SHARP
VC9300
Won't Take Up.
Remove T/u Spools, Clean And Grease. Replace Idler, Greas Underneath.
SHARP
VC9300
Wont Tune To Stations.
Check Aux/tuner Switch Faulty.
SHARP
VC9500
Sound Warble.
Reel Motor Faulty.
SHARP
VC9700
11v And 13v Rails Down.
Check D9008 In P/s. Also Check For Corrosion Of Component Legs Caused By Holding Glue.
SHARP
VC9700
After Several Hrs Picture Pulling At Top.
Check For Rubbing Sound From Drum Bearing.
SHARP
VC9700
Chews Tapes.
Q708 S/c
SHARP
VC9700
Clock Display Too Bright.
Check D6603 S/c If Clock Ic15002 Faulty. Remove C5007 Before Changing Ic15002.
SHARP
VC9700
Clock Dist./flash. Capstan/drum Motors Interm. Start. -
Replace Ic5002.
SHARP
VC9700
Display Goes Dim After 1 Hour.
Check Pr6601 On Audio Board.
SHARP
VC9700
Drum No Go.
L701 On Servo Pcb Or Remove Glue From Q718 And Q719.
SHARP
VC9700
Failure To Accept Tape.
Check Cass In Switch If Ok Q810.
SHARP
VC9700
Head Drum To Go.
Check L701 On Servo Pcb.
SHARP
VC9700
Int Failure To Play.
Check Drum Doesn't Rotate When Faulty Present, E52 Low 1 Volt. Drum Muting Trans Q719 Leaky.
SHARP
VC9700
Int Failure To Record Sound.
Change Relays, Change C648 To .1 Mfd, R693 To 10 K Ohm .25w. Or .01.
SHARP
VC9700
Int Loss Of Colour.
Check Ic301 (sa8063) Overheating. Replace.
SHARP
VC9700
Int Reel Drive.
Dj On Pin 18 Of Ic704.
SHARP
VC9700
Int Wowing In Play.
Check Q710 O/c.
SHARP
VC9700
Intermittently Dead With No Clock Display.
Check Chopper Regulator Chip 19001 (stk722b) Also Q9001.
SHARP
VC9700
Loss Of Field Sync In Record.
Check C542 On Y/c Board Should Be .1 Mfd Not .33 Mfd.
SHARP
VC9700
No Display
4O7 Ptc Ht Feed To -30 Volt And Heater Line
SHARP
VC9700
No Go No Clock
Q5002 Or Circuit Board O/c
SHARP
VC9700
No Line Sync In Visual Search.
Replace Idler And Reel Motor.
SHARP
VC9700
No Operate, No Clock.
Q5002 U/s Or Print To Collector O/c.
SHARP
VC9700
No Pic On Play Or E-e Pic Is On Play.
Glue On Q809 (rec 11v Switch).
SHARP
VC9700
Rf Interference On Low Channels.
1. Unsolder "mgnd". Green Wire At K9005. 2. Unsolder "gnd" Brown Wire At K9003 And Resolder At C9006 "-".
SHARP
VCA101
Int Stops In Rew/ff.
Earth Cassette Holder Slider By Fitting Spring (msprp0113gefj).
SHARP
VCA101
Loading Motor Stops Intermittently
Ic803 Load Motor Driver Ic.
SHARP
VCA101
No Drum Rotation No Drum Afc Apc Ok.
Replace Ic801 Syscon.
SHARP
VCA101
Not Erasing Audio And Not Recording New Audio
Hard Wire Full Erase Head
SHARP
VCA101
Shuts Down In Playback Maybe When Warm.
Check Take Up Hub To Be Stiff Or Seized
SHARP
VCA101
Unit Accepts Tapes Then Ejects Straight Away
Cassette Detect Switch On Top Of Carriage Is Shorted Closed.
SHARP
VCA103
Hum Bars In Record.
D906, D907, D908, D909 High Resistance
SHARP
VCA103
Int Stops In Rew/ff
Hard Wire Full Erasee Head.
SHARP
VCA103
See Vca101
SHARP
VCA103
White Bar Or Distortion Of Tuner Pic. Only Whilst Recording
Check For Faulty Or Leaky Diode In Power Supply. Check D906, D907, D908 And D909.
SHARP
VCA103
Won't Accept Cass. If No Cass. In Unit Turns Off.
Check Operation Of Q901, 2sd1565 In Power Circuit.
SHARP
VCA103
Wont Eject Sometimes.
See Phillips Vr6448
SHARP
VCA105
At Switch On, Loads Then Unloads - Crazy.
Mode Switch, Clean Contracts, Or Replace.
SHARP
VCA105
Back Tension Arm Jams On Unload
Replace Plastic Brackets Parts #52 And #53
SHARP
VCA105
Cassette Jams On Eject
Bend (modify) Pinch Roller Lever Forward 1-1.5 Mil
SHARP
VCA105
Int Rew/ff From Stop Mode
Replace Idler Ngerh1122gezz
SHARP
VCA105
Laces Up And Then Unlaces No Head Switch
Fg Pcb Coil O/c On Bottom Of Motor Spike At Contacts Coat With Laquer
SHARP
VCA105
Power Up Erattic Mechanism
Mode Switch.
SHARP
VCA105
Wont Accept Tape
Change Sensors Pcb To New Type Duntk3194gezz
SHARP
VCA111
At Switch On, Loads Then Unloads - Crazy.
Mode Switch, Clean Contacts, Or Replace.
SHARP
VCA111
Back Tension Arm Jams On Unload.
Plastic Brackets, No: 52 And 53 In Service Manual.
SHARP
VCA111
Cassette Jams On Eject.
Bend Lever On Pinch Roller Forward 1 - 1.5 Mm.
SHARP
VCA111
Int Rew/ff From Stop Mode.
Replace Idler. (ngerh1122gezz).
SHARP
VCA111
Laces Up Then Immediatly Unlaces No H.S.P.
Fg Pcb Coil On Bottom Of Drum Motor O/c. Spike Contracts.
SHARP
VCA111
See Vca105
SHARP
VCA111
Won't Accept Tape.
Change Sensor Pcb To New Type. Duntk3194he00.
SHARP
VCA45
No Capstan Motor Drive.
Replaced Leaking Capacitor On Capstan Motor Pcb. check Tracks Haven't Been Destroyed By Leaking Electrolyte.
SHARP
VCA502
All Functions Ok Except Play.No Capstan Drive.
Capstan Drive Ic X0322ge.
SHARP
VCA502
Eratic Functions When In Rewind,goes F.F.,breaks Tapes.
Display Stays In Rewind....Replace Capstan Motor.
SHARP
VCA502
Int Stops In Rew/ff.
Earth Cassette Holder Slider By Fitting Spring (msprp0113gefj).
SHARP
VCA502
Not Erasing Previous Audio Track.
Hard Wire Full Erase Head.
SHARP
VCA502
See Sharp Vca101
SHARP
VCA505
At Switch On, Loads Then Unloads - Crazy.
Mode Switch, Clean Contacts.
SHARP
VCA505
Back Tension Arm Jams On Unload.
Plastic Brackets, Parts 52 And 53 In Manual.
SHARP
VCA505
Cassette Jams On Eject.
Bend Lever On Pinch Roller Forward 1 - 1.5 Mm.
SHARP
VCA505
Int Rew/ff From Stop Mode.
Replace Idler Ngerh1122gezz.
SHARP
VCA505
Laces Then Immediately Unlaces. No H.S.P.
Fg Pcb Coil On Bottom Of Drum Motor O/c. Spike Contracts.
SHARP
VCA505
Screen Green No Audio In Playback.
No Control Pulse Dirty Heads.
SHARP
VCA505
See Sharp Vca105
SHARP
VCA505
Won't Accept Tape.
Change Sensor Pcb To New Type Duntk3194he00.
SHARP
VCA510
Cassette Jams On Eject.
Bend Lever On Pinch Roller Forward 1 - 1.5mm
SHARP
VCA510
See Sharp Vca105
SHARP
VCA62
No Go After Storm.No Display.
Transistor Q902 2sc2001 Faulty.
SHARP
VCA67
Does Not Pull Tape Back Into Cassette When Unloading. machine Shuts Down Intermittently
Back Tension Band Felt Has Come Off. Band Sticking To Reel. replaced Back Tension Band. Vslbndk1008gezz
SHARP
VCB60
See Vcb20 Service Manual
SHARP
VCD801
Int Stops In Rew/ff.
Earth Cassette Holder Slider By Fitting Spring (msprp-113gefj).
SHARP
VCD801
Not Erase Previous Audio Track.
Hard Wire Full Erase Head.
SHARP
VCD805
Cassette Jams On Eject.
Bend Lever On Pinch Roller Forward 1 - 1.5 Mm.
SHARP
VCD805
See Vca101
SHARP
VCH83X
Reel Sensor Has No Pulse And Has 12v Where It Should Not!
Found Connectors On Bus Board Between Power Supply And Eject To Have Corrosion From Liquid.
SHARP
VCH851
Int Stops In Rew/ff.
Earth Cassette Holder Slider By Fitting Spring (msprpo113gefj)
SHARP
VCH851
Not Erasing Previous Audio Track.
Hard Wire Full Erase Head.
SHARP
VCH851
See Vca101
SHARP
VCH855
All Tape Functions Stop After Several Seconds.
Remove And Clean T.U. Reel Sensor, Mounted On Chassis Pcb.
SHARP
VCH87
Picture O.K. Hi-fi Audio O.K. In P/b And Rec. machine Will Not Play Back Linear Audio.
Replace Faulty Q6306 Transistor With Bc548(check Pin Conn). q6306 Is Surface Mount And Lives On Audio Sub Board(with The Surface Mount Processor).
SHARP
VCP4100
Capstan Runs All The Time.
C615 Faulty.
SHARP
VCP4100
Capstan Unlocked.
Change R239 To 390 Ohm, C239 To 22µf, R237 To 2.2m.
SHARP
VCP4100
Chews Tapes.
Remove T/u Guide Arm Unit.
SHARP
VCP4100
Colour Flickers.
X302 Faulty.
SHARP
VCP4100
Colour Patterning, Int Colour.
Remove Earth From Power Lead.
SHARP
VCP4100
D209 Cooks.
Loom To Dd Shorted To Earth.
SHARP
VCP4100
Improve Dew Detection.
Change R608 To 56k.
SHARP
VCP4100
Improve Pg Shift.
Change R215/216 To 18k. Change Vr201/202 To 33k.
SHARP
VCP4100
Int Colour.
Upc1536c Faulty.
SHARP
VCP4100
Int Servo Lock.
X301 Must Use Original Type.
SHARP
VCP4100
Looks Like Heads Faulty.
C329 Faulty.
SHARP
VCP4100
Looks Like Heads Faulty.
C306, C301, C3095 Faulty.
SHARP
VCP4100
No Capstan Drive.
C615 Faulty.
SHARP
VCP4100
No Colour.
C337, C347 Faulty.
SHARP
VCP4100
No Picture On Play.
C306 Faulty.
SHARP
VCP4100
Noise Bar Thru Pic Every 3 Minutes.
C229 Faulty.
SHARP
VCP4100
Patterning On Picture.
Add Earth To Head Leads, Check Lead Dress To Heads.
SHARP
VCP4100
Pic Goes Off Like Heads When Hot.
C105, Or Dj On Q206 (headswitch).
SHARP
VCP4100
Pic Noise In Play, As Through In Cue.
C207 Faulty.
SHARP
VCP4100
Pic Skew In Cue/review.
Change C3a0 To .22µf.
SHARP
VCP4100
Pic Weak, Horiz Bars.
C387 Faulty.
SHARP
VCP4100
Picture Beat And Patterning.
C347 Faulty.
SHARP
VCP4100
Stops After 2 Secs In Play.
Fit New Reel Sensor. Dont Modify.
SHARP
VCP4100
Tracking Doesn't Adjust.
C205 Fautly.
SHARP
VCP4100
White Flicker Noise.
C317, C318 Fautly.
SHARP
VCT510
At Switch On, Loads Then Unloads - Crazy.
Mode Switch, Clean Contacts.
SHARP
VCT510
Back Tension Arm Jams On Unload.
Plastic Brackets, Parts 52 And 53 In Manual.
SHARP
VCT510
Laces Then Immediatly Unlaces. No H.S.P.
Fg Pcb Coil On Bottom Of Drum Motoro/c. Spike Contacts, Coats With Laquer.
SHARP
VCT510
See Sharp Vca105
SHARP
VCT510
Won't Accept Tape.
Change Sensor Pcb To New Type. Duntk3194he00.
SHARP
VLC6100
Snowy Picture, Sometimes 1/2 Screen
Replaced Servo Smd Ic. Ir3p71 Lmir3p711 On Main Board
SHARP
VLC670
No Audio In Play Or Record Modes
Audio Hybrib.?? Lmrhiz0093tazz
SHARP
VLC770
No Power.
C 802 On Main Syscon Pcb 10µ/16v Smd Cap . Dcdc Converter And Audio Hybrib
SHARP
VLC8000
Ghosting In Playback
Unit Needs To Be Recapped. c2206 47 µ6v Near Connector Bc On Y/c Pcb
SHARP
VLM78E
No Colour From Recorded Tape, Pb Ok
10 µ Caps C420. Also 480,411,416. 22 µ Appeared To Be Ok, But Was Replaced.
SHARP
VLM78E
See Sharp Vlm4x Similar
SHARP
VLM78E
See Vlm4x
Similar To Vlm4x
SHARP
XC30
No Video
Check If Nothing At Tp3. Check Q102 Collector Volts Low (18v). Target Connector To Screening Shield S/c.
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